(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.597)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0175)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.196)
				(material "7628")
				(epsilon_r 4.74)
				(loss_tangent 0)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.03)
				(material "FR4")
				(epsilon_r 4.6)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.196)
				(material "7628")
				(epsilon_r 4.74)
				(loss_tangent 0)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0175)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J5-Pin_3)")
	(net 2 "Net-(D9-K)")
	(net 3 "Net-(D8-K)")
	(net 4 "Net-(J5-Pin_2)")
	(net 5 "Net-(J5-Pin_1)")
	(net 6 "Net-(D7-K)")
	(net 7 "Net-(C4-Pad2)")
	(net 8 "GND")
	(net 9 "Net-(U4-FB)")
	(net 10 "3.3V{slash}2A")
	(net 11 "Net-(U3-USBDP)")
	(net 12 "Net-(D4-K)")
	(net 13 "+3.3V")
	(net 14 "Net-(J1-Pin_2)")
	(net 15 "Net-(U3-USBDM)")
	(net 16 "Net-(D5-K)")
	(net 17 "Net-(D2-K)")
	(net 18 "Net-(U3-CBUS0)")
	(net 19 "Net-(J5-Pin_8)")
	(net 20 "Net-(D14-K)")
	(net 21 "Net-(J5-Pin_7)")
	(net 22 "Net-(D13-K)")
	(net 23 "Net-(D12-K)")
	(net 24 "Net-(J5-Pin_6)")
	(net 25 "Net-(D11-K)")
	(net 26 "Net-(J5-Pin_5)")
	(net 27 "Net-(J5-Pin_4)")
	(net 28 "Net-(D10-K)")
	(net 29 "Net-(D1-K)")
	(net 30 "Net-(U4-COMP)")
	(net 31 "+12V")
	(net 32 "Net-(U4-SS)")
	(net 33 "unconnected-(U4-EN-Pad7)")
	(net 34 "Net-(U4-BS)")
	(net 35 "unconnected-(U6-Pad13)")
	(net 36 "unconnected-(U6-Pad9)")
	(net 37 "+5V")
	(net 38 "TX")
	(net 39 "unconnected-(U6-Pad11)")
	(net 40 "unconnected-(U6-Pad3)")
	(net 41 "unconnected-(U6-Pad5)")
	(net 42 "RX")
	(net 43 "unconnected-(U1-PB10-Pad69)")
	(net 44 "Net-(U1-VREF+)")
	(net 45 "unconnected-(U1-PC0-Pad26)")
	(net 46 "Net-(C27-Pad1)")
	(net 47 "Net-(U1-PE7)")
	(net 48 "unconnected-(U1-PB14-Pad75)")
	(net 49 "unconnected-(U1-PB7-Pad137)")
	(net 50 "unconnected-(U1-PE13-Pad66)")
	(net 51 "Net-(J6-Pin_8)")
	(net 52 "Net-(J6-Pin_7)")
	(net 53 "unconnected-(U1-PH0-Pad23)")
	(net 54 "unconnected-(U1-PF11-Pad49)")
	(net 55 "unconnected-(U1-PG11-Pad126)")
	(net 56 "unconnected-(U1-PA8-Pad100)")
	(net 57 "unconnected-(U1-PE10-Pad63)")
	(net 58 "unconnected-(U1-PE9-Pad60)")
	(net 59 "unconnected-(U1-PD4-Pad118)")
	(net 60 "unconnected-(U1-PD7-Pad123)")
	(net 61 "unconnected-(U1-PB2-Pad48)")
	(net 62 "unconnected-(U1-PE4-Pad3)")
	(net 63 "unconnected-(U1-PF2-Pad12)")
	(net 64 "unconnected-(U1-PE14-Pad67)")
	(net 65 "unconnected-(U1-PG15-Pad132)")
	(net 66 "unconnected-(U1-PG0-Pad56)")
	(net 67 "unconnected-(U1-PF3-Pad13)")
	(net 68 "unconnected-(U1-PF14-Pad54)")
	(net 69 "unconnected-(U1-PG1-Pad57)")
	(net 70 "unconnected-(U1-PC12-Pad113)")
	(net 71 "unconnected-(U1-PC13-Pad7)")
	(net 72 "unconnected-(U1-PF4-Pad14)")
	(net 73 "unconnected-(U1-PD2-Pad116)")
	(net 74 "unconnected-(U1-PF0-Pad10)")
	(net 75 "unconnected-(U1-PD1-Pad115)")
	(net 76 "unconnected-(U1-PF15-Pad55)")
	(net 77 "Net-(J6-Pin_4)")
	(net 78 "unconnected-(U1-PC15-Pad9)")
	(net 79 "unconnected-(U1-PF5-Pad15)")
	(net 80 "Net-(J6-Pin_5)")
	(net 81 "unconnected-(U1-PE12-Pad65)")
	(net 82 "Net-(U1-PE8)")
	(net 83 "unconnected-(U1-PA9-Pad101)")
	(net 84 "unconnected-(U1-PD15-Pad86)")
	(net 85 "unconnected-(U1-PE1-Pad142)")
	(net 86 "unconnected-(U1-PB4(NJTRST)-Pad134)")
	(net 87 "unconnected-(U1-PF13-Pad53)")
	(net 88 "unconnected-(U1-PG14-Pad129)")
	(net 89 "unconnected-(U1-PE0-Pad141)")
	(net 90 "unconnected-(U1-PB12-Pad73)")
	(net 91 "unconnected-(U1-PF12-Pad50)")
	(net 92 "unconnected-(U1-PD6-Pad122)")
	(net 93 "unconnected-(U1-PE3-Pad2)")
	(net 94 "unconnected-(U1-PE11-Pad64)")
	(net 95 "unconnected-(U1-PC3_C-Pad29)")
	(net 96 "unconnected-(U1-PA13(JTMS-Pad105)")
	(net 97 "unconnected-(U1-PA0-Pad34)")
	(net 98 "unconnected-(U1-PH1-Pad24)")
	(net 99 "unconnected-(U1-PF1-Pad11)")
	(net 100 "unconnected-(U1-PC2_C-Pad28)")
	(net 101 "Net-(J6-Pin_6)")
	(net 102 "unconnected-(U1-PB8-Pad139)")
	(net 103 "unconnected-(U1-PD13-Pad82)")
	(net 104 "unconnected-(U1-PC4-Pad44)")
	(net 105 "unconnected-(U1-PD0-Pad114)")
	(net 106 "unconnected-(U1-BOOT0-Pad138)")
	(net 107 "unconnected-(U1-PF7-Pad19)")
	(net 108 "unconnected-(U1-PF10-Pad22)")
	(net 109 "unconnected-(U1-PC1-Pad27)")
	(net 110 "unconnected-(U1-PB11-Pad70)")
	(net 111 "unconnected-(U1-PA3-Pad37)")
	(net 112 "unconnected-(U1-PE2-Pad1)")
	(net 113 "unconnected-(U1-PC8-Pad98)")
	(net 114 "unconnected-(U1-PB9-Pad140)")
	(net 115 "unconnected-(U1-PC14-Pad8)")
	(net 116 "unconnected-(U1-NRST-Pad25)")
	(net 117 "unconnected-(U1-PG13-Pad128)")
	(net 118 "unconnected-(U1-PA11-Pad103)")
	(net 119 "unconnected-(U1-PD3-Pad117)")
	(net 120 "unconnected-(U1-PG12-Pad127)")
	(net 121 "unconnected-(U1-PF6-Pad18)")
	(net 122 "unconnected-(U1-PE6-Pad5)")
	(net 123 "unconnected-(U1-PD11-Pad80)")
	(net 124 "unconnected-(U1-PF9-Pad21)")
	(net 125 "unconnected-(U1-PG10-Pad125)")
	(net 126 "unconnected-(U1-PD10-Pad79)")
	(net 127 "unconnected-(U1-PA1-Pad35)")
	(net 128 "unconnected-(U1-PE5-Pad4)")
	(net 129 "unconnected-(U1-PB13-Pad74)")
	(net 130 "unconnected-(U1-PD5-Pad119)")
	(net 131 "unconnected-(U1-PC9-Pad99)")
	(net 132 "unconnected-(U1-PDR_ON-Pad143)")
	(net 133 "unconnected-(U1-PA2-Pad36)")
	(net 134 "unconnected-(U1-PD14-Pad85)")
	(net 135 "unconnected-(U1-PF8-Pad20)")
	(net 136 "unconnected-(U1-PB15-Pad76)")
	(net 137 "unconnected-(U1-PD8-Pad77)")
	(net 138 "unconnected-(U1-PE15-Pad68)")
	(net 139 "unconnected-(U1-PA10-Pad102)")
	(net 140 "unconnected-(U1-PB3(JTDO-Pad133)")
	(net 141 "unconnected-(U1-PA14(JTCK-Pad109)")
	(net 142 "unconnected-(U1-PD12-Pad81)")
	(net 143 "unconnected-(U1-PC7-Pad97)")
	(net 144 "unconnected-(U1-PA15(JTDI)-Pad110)")
	(net 145 "Net-(J6-Pin_3)")
	(net 146 "unconnected-(U1-PB6-Pad136)")
	(net 147 "unconnected-(U1-PB5-Pad135)")
	(net 148 "unconnected-(U1-PA12-Pad104)")
	(net 149 "unconnected-(U1-PD9-Pad78)")
	(net 150 "unconnected-(U1-PC5-Pad45)")
	(net 151 "Net-(D2-A)")
	(net 152 "unconnected-(U3-~{RTS}{slash}D2-Pad8)")
	(net 153 "unconnected-(U3-~{CTS}{slash}D3-Pad11)")
	(net 154 "unconnected-(U2-Shield-Pad5)")
	(net 155 "unconnected-(U2-Shield-Pad5)_1")
	(net 156 "unconnected-(J6-Pin_9-Pad9)")
	(net 157 "unconnected-(J6-Pin_10-Pad10)")
	(net 158 "unconnected-(J6-Pin_13-Pad13)")
	(net 159 "unconnected-(J6-Pin_12-Pad12)")
	(net 160 "unconnected-(J6-Pin_14-Pad14)")
	(net 161 "unconnected-(J6-Pin_11-Pad11)")
	(net 162 "unconnected-(J6-Pin_20-Pad20)")
	(net 163 "unconnected-(J6-Pin_19-Pad19)")
	(net 164 "unconnected-(U7-3A-Pad9)")
	(net 165 "unconnected-(U7-3OE-Pad10)")
	(net 166 "unconnected-(U7-3Y-Pad8)")
	(net 167 "unconnected-(U1-PG9-Pad124)")
	(net 168 "unconnected-(U1-PC11-Pad112)")
	(net 169 "unconnected-(U1-PC10-Pad111)")
	(net 170 "unconnected-(U7-4A-Pad12)")
	(net 171 "TXD")
	(net 172 "unconnected-(U7-4OE-Pad13)")
	(net 173 "RXD")
	(net 174 "TXEN")
	(net 175 "unconnected-(U7-4Y-Pad11)")
	(net 176 "RXEN")
	(net 177 "unconnected-(U6-Pad2)")
	(net 178 "unconnected-(U6-Pad1)")
	(net 179 "Net-(PS1--Vin)")
	(net 180 "Net-(PS1-+Vin)")
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 256.13 15.97 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 32 "Net-(U4-SS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 73)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 28 "Net-(D10-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(J5-Pin_4)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 261.13 20.97 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 10 "3.3V{slash}2A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 267.13 22.97)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 9 "Net-(U4-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_A_CONNFLY_DS1095-WNR0"
		(layer "F.Cu")
		(at 282.9775 132 -90)
		(descr "http://www.connfly.com/userfiles/image/UpLoadFile/File/2013/5/6/DS1095.pdf")
		(tags "USB-A receptacle horizontal through-hole")
		(property "Reference" "U2"
			(at -1.95 -2.35 90)
			(layer "F.SilkS")
		)
		(property "Value" "USB_A"
			(at 3.5 7 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_USB:USB_A_CONNFLY_DS1095-WNR0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB Type A connector"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.524 1.524)
			(drill 0.92)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+3.3V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.524 1.524)
			(drill 0.92)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D5-K)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 4.5 0 270)
			(size 1.524 1.524)
			(drill 0.92)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D4-K)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 7 0 270)
			(size 1.524 1.524)
			(drill 0.92)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole circle
			(at -3.07 2.71 270)
			(size 3.5 3.5)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 155 "unconnected-(U2-Shield-Pad5)_1")
			(pinfunction "Shield")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole circle
			(at 10.07 2.71 270)
			(size 3.5 3.5)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "unconnected-(U2-Shield-Pad5)")
			(pinfunction "Shield")
			(pintype "passive+no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_CONNFLY_DS1095-WNR0.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 267.13 17.97)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "21k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 9 "Net-(U4-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 10 "3.3V{slash}2A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
		(layer "F.Cu")
		(at 257.875 135.7 -90)
		(descr "WDFN, 12 Pin (https://www.diodes.com/assets/Datasheets/PAM2306.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "WDFN NoLead")
		(property "Reference" "U3"
			(at 0 -2.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "FT234XD"
			(at 0 2.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2024/05/DS_FT234XD.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Full Speed USB to Basic UART, WDFN-12"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WDFN*1EP*3x3mm*P0.45mm*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.425 -0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.425 0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.425 -0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.425 0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.45 -1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U3-USBDM)")
			(pinfunction "USBDM")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.45 -0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "Net-(D2-A)")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.45 -0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "Net-(D2-A)")
			(pinfunction "3V3OUT")
			(pintype "power_out")
		)
		(pad "4" smd roundrect
			(at -1.45 0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.45 0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -1.45 1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U3-CBUS0)")
			(pinfunction "CBUS0")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 1.45 1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U1-PE7)")
			(pinfunction "TXD/D0")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 1.45 0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "unconnected-(U3-~{RTS}{slash}D2-Pad8)")
			(pinfunction "~{RTS}/D2")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd roundrect
			(at 1.45 0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "Net-(D2-A)")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 1.45 -0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "Net-(U1-PE8)")
			(pinfunction "RXD/D1")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 1.45 -0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "unconnected-(U3-~{CTS}{slash}D3-Pad11)")
			(pinfunction "~{CTS}/D3")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd roundrect
			(at 1.45 -1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U3-USBDP)")
			(pinfunction "USBDP")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.7 2.5)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 254.13 26.97 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7nF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 30 "Net-(U4-COMP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 7 "Net-(C4-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Bourns_SRF0905_6.0x9.2mm"
		(layer "F.Cu")
		(at 159 29.27)
		(descr "https://www.bourns.com/docs/Product-Datasheets/SRF0905.pdf")
		(tags "Line Filter")
		(property "Reference" "FL1"
			(at 0 -4 180)
			(layer "F.SilkS")
		)
		(property "Value" "(744226S)"
			(at 0 4 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Filter:Filter_Bourns_SRF0905_6.0x9.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "EMI 2-inductor common mode filter"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L_* L_CommonMode*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.75 -1.27)
			(size 2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+12V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.75 1.27)
			(size 2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 180 "Net-(PS1-+Vin)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 3.75 1.27)
			(size 2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 3.75 -1.27)
			(size 2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 179 "Net-(PS1--Vin)")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Filter.3dshapes/Filter_Bourns_SRF0905_6.0x9.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 267.5 130.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(U3-CBUS0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 79)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 3 "Net-(D8-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(J5-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 254.5 138.4875 -90)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.82 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0 270)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 17 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4875 0 270)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 151 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_1.00mm:PinSocket_1x20_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 144 141 90)
		(descr "Through hole straight socket strip, 1x20, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated")
		(tags "Through hole socket strip THT 1x20 1.00mm single row")
		(property "Reference" "J6"
			(at -0.29 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "Display Socket"
			(at -0.29 21.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_1.00mm:PinSocket_1x20_P1.00mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.29 9.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(J6-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "Net-(J6-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 4 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "Net-(J6-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 5 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "Net-(J6-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 6 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J6-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 7 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J6-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 8 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 156 "unconnected-(J6-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole oval
			(at 0 9 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "unconnected-(J6-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 10 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 161 "unconnected-(J6-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive+no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 11 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 159 "unconnected-(J6-Pin_12-Pad12)")
			(pinfunction "Pin_12")
			(pintype "passive+no_connect")
		)
		(pad "13" thru_hole oval
			(at 0 12 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 158 "unconnected-(J6-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 13 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 160 "unconnected-(J6-Pin_14-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
		)
		(pad "15" thru_hole oval
			(at 0 14 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 15 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+3.3V")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 16 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 0 17 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 18 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "unconnected-(J6-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole oval
			(at 0 19 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 162 "unconnected-(J6-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_1.00mm.3dshapes/PinSocket_1x20_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 79.285 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 3 "Net-(D8-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 64.285 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D13"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 22 "Net-(D13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 76)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(D9-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "Net-(J5-Pin_3)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 267.5 136.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 11 "Net-(U3-USBDP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D4-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 249.13 28.4575 -90)
		(descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D1"
			(at 0 -1.82 90)
			(layer "F.SilkS")
		)
		(property "Value" "B340"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0 270)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 29 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4875 0 270)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 73.25 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D10"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 28 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 82)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(D7-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "Net-(J5-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 267.5 134.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 15 "Net-(U3-USBDM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 16 "Net-(D5-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 266.5 127 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 8 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(U3-CBUS0)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 224.75 56.215 90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D15"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 90)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 38 "TX")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 90)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x03_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 119 14 -90)
		(descr "Through hole straight pin header, 1x03, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x03 1.00mm single row")
		(property "Reference" "J1"
			(at 0 -1.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "Motor Conn1"
			(at 0 3.56 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_1.00mm:PinHeader_1x03_P1.00mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2 270)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x03_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 67)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 23 "Net-(D12-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(J5-Pin_6)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 82.285 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 6 "Net-(D7-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 251.475 21.095)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MP2303ADN"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/MP2303A_r1.1.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Synchronous Rectified 3A, 28V, 360kHz Step-Down Converter, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*1EP*3.9x4.9mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U4-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(D1-K)")
			(pinfunction "SW")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U4-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U4-COMP)")
			(pinfunction "COMP")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "unconnected-(U4-EN-Pad7)")
			(pinfunction "EN")
			(pintype "input+no_connect")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U4-SS)")
			(pinfunction "SS")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 61)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 20 "Net-(D14-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 19 "Net-(J5-Pin_8)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_1.27mm:PinSocket_1x08_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 282.975 78.54 180)
		(descr "Through hole straight socket strip, 1x08, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x08 1.27mm single row")
		(property "Reference" "J5"
			(at 0 -2.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Keypad Socket"
			(at -3 4.8 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_1.27mm:PinSocket_1x08_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 4.445 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 1.27 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 3.81 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J5-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 6.35 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J5-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J5-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 8.89 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J5-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x08_P1.27mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 134.725 56.54)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at 0 -5.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC04"
			(at 0 5.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT04.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Hex Inverter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SSOP?14* TSSOP?14*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "unconnected-(U6-Pad1)")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "unconnected-(U6-Pad2)")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U6-Pad3)")
			(pintype "input+no_connect")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "unconnected-(U6-Pad5)")
			(pintype "input+no_connect")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "unconnected-(U6-Pad9)")
			(pintype "input+no_connect")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U6-Pad11)")
			(pintype "input+no_connect")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(U6-Pad13)")
			(pintype "input+no_connect")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 61.285 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D14"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0.235 1.35 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 20 "Net-(D14-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-144_20x20mm_P0.5mm"
		(layer "F.Cu")
		(at 220 77)
		(descr "LQFP, 144 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=425), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U1"
			(at 0 -12.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "STM32H723ZGTx"
			(at 0 12.35 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h723zg.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M7 MCU, 1024KB flash, 564KB RAM, 550 MHz, 1.62-3.6V, 114 GPIO, LQFP144"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LQFP*20x20mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -10.6625 -8.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "unconnected-(U1-PE2-Pad1)")
			(pinfunction "PE2")
			(pintype "bidirectional+no_connect")
		)
		(pad "2" smd roundrect
			(at -10.6625 -8.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "unconnected-(U1-PE3-Pad2)")
			(pinfunction "PE3")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd roundrect
			(at -10.6625 -7.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "unconnected-(U1-PE4-Pad3)")
			(pinfunction "PE4")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd roundrect
			(at -10.6625 -7.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "unconnected-(U1-PE5-Pad4)")
			(pinfunction "PE5")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -10.6625 -6.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "unconnected-(U1-PE6-Pad5)")
			(pinfunction "PE6")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" smd roundrect
			(at -10.6625 -6.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VBAT")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -10.6625 -5.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "unconnected-(U1-PC13-Pad7)")
			(pinfunction "PC13")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd roundrect
			(at -10.6625 -5.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "unconnected-(U1-PC14-Pad8)")
			(pinfunction "PC14")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd roundrect
			(at -10.6625 -4.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "unconnected-(U1-PC15-Pad9)")
			(pinfunction "PC15")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" smd roundrect
			(at -10.6625 -4.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "unconnected-(U1-PF0-Pad10)")
			(pinfunction "PF0")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd roundrect
			(at -10.6625 -3.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "unconnected-(U1-PF1-Pad11)")
			(pinfunction "PF1")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd roundrect
			(at -10.6625 -3.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "unconnected-(U1-PF2-Pad12)")
			(pinfunction "PF2")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" smd roundrect
			(at -10.6625 -2.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "unconnected-(U1-PF3-Pad13)")
			(pinfunction "PF3")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" smd roundrect
			(at -10.6625 -2.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "unconnected-(U1-PF4-Pad14)")
			(pinfunction "PF4")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd roundrect
			(at -10.6625 -1.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "unconnected-(U1-PF5-Pad15)")
			(pinfunction "PF5")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" smd roundrect
			(at -10.6625 -1.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at -10.6625 -0.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at -10.6625 -0.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "unconnected-(U1-PF6-Pad18)")
			(pinfunction "PF6")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" smd roundrect
			(at -10.6625 0.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "unconnected-(U1-PF7-Pad19)")
			(pinfunction "PF7")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" smd roundrect
			(at -10.6625 0.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "unconnected-(U1-PF8-Pad20)")
			(pinfunction "PF8")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd roundrect
			(at -10.6625 1.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 124 "unconnected-(U1-PF9-Pad21)")
			(pinfunction "PF9")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd roundrect
			(at -10.6625 1.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "unconnected-(U1-PF10-Pad22)")
			(pinfunction "PF10")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" smd roundrect
			(at -10.6625 2.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U1-PH0-Pad23)")
			(pinfunction "PH0")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd roundrect
			(at -10.6625 2.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "unconnected-(U1-PH1-Pad24)")
			(pinfunction "PH1")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd roundrect
			(at -10.6625 3.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "unconnected-(U1-NRST-Pad25)")
			(pinfunction "NRST")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -10.6625 3.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U1-PC0-Pad26)")
			(pinfunction "PC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd roundrect
			(at -10.6625 4.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "unconnected-(U1-PC1-Pad27)")
			(pinfunction "PC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd roundrect
			(at -10.6625 4.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "unconnected-(U1-PC2_C-Pad28)")
			(pinfunction "PC2_C")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd roundrect
			(at -10.6625 5.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 95 "unconnected-(U1-PC3_C-Pad29)")
			(pinfunction "PC3_C")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" smd roundrect
			(at -10.6625 5.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "31" smd roundrect
			(at -10.6625 6.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSSA")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at -10.6625 6.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "Net-(U1-VREF+)")
			(pinfunction "VREF+")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at -10.6625 7.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "34" smd roundrect
			(at -10.6625 7.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "unconnected-(U1-PA0-Pad34)")
			(pinfunction "PA0")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd roundrect
			(at -10.6625 8.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "unconnected-(U1-PA1-Pad35)")
			(pinfunction "PA1")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" smd roundrect
			(at -10.6625 8.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 133 "unconnected-(U1-PA2-Pad36)")
			(pinfunction "PA2")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" smd roundrect
			(at -8.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "unconnected-(U1-PA3-Pad37)")
			(pinfunction "PA3")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd roundrect
			(at -8.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "39" smd roundrect
			(at -7.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at -7.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "Net-(J6-Pin_6)")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at -6.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "Net-(J6-Pin_3)")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at -6.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "Net-(J6-Pin_4)")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at -5.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(J6-Pin_5)")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at -5.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "unconnected-(U1-PC4-Pad44)")
			(pinfunction "PC4")
			(pintype "bidirectional+no_connect")
		)
		(pad "45" smd roundrect
			(at -4.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "unconnected-(U1-PC5-Pad45)")
			(pinfunction "PC5")
			(pintype "bidirectional+no_connect")
		)
		(pad "46" smd roundrect
			(at -4.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "Net-(J6-Pin_7)")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at -3.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "Net-(J6-Pin_8)")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at -3.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "unconnected-(U1-PB2-Pad48)")
			(pinfunction "PB2")
			(pintype "bidirectional+no_connect")
		)
		(pad "49" smd roundrect
			(at -2.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U1-PF11-Pad49)")
			(pinfunction "PF11")
			(pintype "bidirectional+no_connect")
		)
		(pad "50" smd roundrect
			(at -2.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "unconnected-(U1-PF12-Pad50)")
			(pinfunction "PF12")
			(pintype "bidirectional+no_connect")
		)
		(pad "51" smd roundrect
			(at -1.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "52" smd roundrect
			(at -1.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "53" smd roundrect
			(at -0.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "unconnected-(U1-PF13-Pad53)")
			(pinfunction "PF13")
			(pintype "bidirectional+no_connect")
		)
		(pad "54" smd roundrect
			(at -0.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "unconnected-(U1-PF14-Pad54)")
			(pinfunction "PF14")
			(pintype "bidirectional+no_connect")
		)
		(pad "55" smd roundrect
			(at 0.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "unconnected-(U1-PF15-Pad55)")
			(pinfunction "PF15")
			(pintype "bidirectional+no_connect")
		)
		(pad "56" smd roundrect
			(at 0.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "unconnected-(U1-PG0-Pad56)")
			(pinfunction "PG0")
			(pintype "bidirectional+no_connect")
		)
		(pad "57" smd roundrect
			(at 1.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "unconnected-(U1-PG1-Pad57)")
			(pinfunction "PG1")
			(pintype "bidirectional+no_connect")
		)
		(pad "58" smd roundrect
			(at 1.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U1-PE7)")
			(pinfunction "PE7")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at 2.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "Net-(U1-PE8)")
			(pinfunction "PE8")
			(pintype "bidirectional")
		)
		(pad "60" smd roundrect
			(at 2.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U1-PE9-Pad60)")
			(pinfunction "PE9")
			(pintype "bidirectional+no_connect")
		)
		(pad "61" smd roundrect
			(at 3.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "62" smd roundrect
			(at 3.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "63" smd roundrect
			(at 4.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U1-PE10-Pad63)")
			(pinfunction "PE10")
			(pintype "bidirectional+no_connect")
		)
		(pad "64" smd roundrect
			(at 4.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "unconnected-(U1-PE11-Pad64)")
			(pinfunction "PE11")
			(pintype "bidirectional+no_connect")
		)
		(pad "65" smd roundrect
			(at 5.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "unconnected-(U1-PE12-Pad65)")
			(pinfunction "PE12")
			(pintype "bidirectional+no_connect")
		)
		(pad "66" smd roundrect
			(at 5.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(U1-PE13-Pad66)")
			(pinfunction "PE13")
			(pintype "bidirectional+no_connect")
		)
		(pad "67" smd roundrect
			(at 6.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "unconnected-(U1-PE14-Pad67)")
			(pinfunction "PE14")
			(pintype "bidirectional+no_connect")
		)
		(pad "68" smd roundrect
			(at 6.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "unconnected-(U1-PE15-Pad68)")
			(pinfunction "PE15")
			(pintype "bidirectional+no_connect")
		)
		(pad "69" smd roundrect
			(at 7.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "unconnected-(U1-PB10-Pad69)")
			(pinfunction "PB10")
			(pintype "bidirectional+no_connect")
		)
		(pad "70" smd roundrect
			(at 7.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 110 "unconnected-(U1-PB11-Pad70)")
			(pinfunction "PB11")
			(pintype "bidirectional+no_connect")
		)
		(pad "71" smd roundrect
			(at 8.25 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "Net-(C27-Pad1)")
			(pinfunction "VCAP")
			(pintype "power_out")
		)
		(pad "72" smd roundrect
			(at 8.75 10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "73" smd roundrect
			(at 10.6625 8.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "unconnected-(U1-PB12-Pad73)")
			(pinfunction "PB12")
			(pintype "bidirectional+no_connect")
		)
		(pad "74" smd roundrect
			(at 10.6625 8.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 129 "unconnected-(U1-PB13-Pad74)")
			(pinfunction "PB13")
			(pintype "bidirectional+no_connect")
		)
		(pad "75" smd roundrect
			(at 10.6625 7.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U1-PB14-Pad75)")
			(pinfunction "PB14")
			(pintype "bidirectional+no_connect")
		)
		(pad "76" smd roundrect
			(at 10.6625 7.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 136 "unconnected-(U1-PB15-Pad76)")
			(pinfunction "PB15")
			(pintype "bidirectional+no_connect")
		)
		(pad "77" smd roundrect
			(at 10.6625 6.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 137 "unconnected-(U1-PD8-Pad77)")
			(pinfunction "PD8")
			(pintype "bidirectional+no_connect")
		)
		(pad "78" smd roundrect
			(at 10.6625 6.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 149 "unconnected-(U1-PD9-Pad78)")
			(pinfunction "PD9")
			(pintype "bidirectional+no_connect")
		)
		(pad "79" smd roundrect
			(at 10.6625 5.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "unconnected-(U1-PD10-Pad79)")
			(pinfunction "PD10")
			(pintype "bidirectional+no_connect")
		)
		(pad "80" smd roundrect
			(at 10.6625 5.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 123 "unconnected-(U1-PD11-Pad80)")
			(pinfunction "PD11")
			(pintype "bidirectional+no_connect")
		)
		(pad "81" smd roundrect
			(at 10.6625 4.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 142 "unconnected-(U1-PD12-Pad81)")
			(pinfunction "PD12")
			(pintype "bidirectional+no_connect")
		)
		(pad "82" smd roundrect
			(at 10.6625 4.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "unconnected-(U1-PD13-Pad82)")
			(pinfunction "PD13")
			(pintype "bidirectional+no_connect")
		)
		(pad "83" smd roundrect
			(at 10.6625 3.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "84" smd roundrect
			(at 10.6625 3.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "85" smd roundrect
			(at 10.6625 2.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 134 "unconnected-(U1-PD14-Pad85)")
			(pinfunction "PD14")
			(pintype "bidirectional+no_connect")
		)
		(pad "86" smd roundrect
			(at 10.6625 2.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "unconnected-(U1-PD15-Pad86)")
			(pinfunction "PD15")
			(pintype "bidirectional+no_connect")
		)
		(pad "87" smd roundrect
			(at 10.6625 1.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D7-K)")
			(pinfunction "PG2")
			(pintype "bidirectional")
		)
		(pad "88" smd roundrect
			(at 10.6625 1.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(D8-K)")
			(pinfunction "PG3")
			(pintype "bidirectional")
		)
		(pad "89" smd roundrect
			(at 10.6625 0.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(D9-K)")
			(pinfunction "PG4")
			(pintype "bidirectional")
		)
		(pad "90" smd roundrect
			(at 10.6625 0.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(D10-K)")
			(pinfunction "PG5")
			(pintype "bidirectional")
		)
		(pad "91" smd roundrect
			(at 10.6625 -0.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D11-K)")
			(pinfunction "PG6")
			(pintype "bidirectional")
		)
		(pad "92" smd roundrect
			(at 10.6625 -0.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(D12-K)")
			(pinfunction "PG7")
			(pintype "bidirectional")
		)
		(pad "93" smd roundrect
			(at 10.6625 -1.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(D13-K)")
			(pinfunction "PG8")
			(pintype "bidirectional")
		)
		(pad "94" smd roundrect
			(at 10.6625 -1.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "95" smd roundrect
			(at 10.6625 -2.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD33USB")
			(pintype "power_in")
		)
		(pad "96" smd roundrect
			(at 10.6625 -2.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D14-K)")
			(pinfunction "PC6")
			(pintype "bidirectional")
		)
		(pad "97" smd roundrect
			(at 10.6625 -3.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 143 "unconnected-(U1-PC7-Pad97)")
			(pinfunction "PC7")
			(pintype "bidirectional+no_connect")
		)
		(pad "98" smd roundrect
			(at 10.6625 -3.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "unconnected-(U1-PC8-Pad98)")
			(pinfunction "PC8")
			(pintype "bidirectional+no_connect")
		)
		(pad "99" smd roundrect
			(at 10.6625 -4.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "unconnected-(U1-PC9-Pad99)")
			(pinfunction "PC9")
			(pintype "bidirectional+no_connect")
		)
		(pad "100" smd roundrect
			(at 10.6625 -4.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U1-PA8-Pad100)")
			(pinfunction "PA8")
			(pintype "bidirectional+no_connect")
		)
		(pad "101" smd roundrect
			(at 10.6625 -5.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "unconnected-(U1-PA9-Pad101)")
			(pinfunction "PA9")
			(pintype "bidirectional+no_connect")
		)
		(pad "102" smd roundrect
			(at 10.6625 -5.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 139 "unconnected-(U1-PA10-Pad102)")
			(pinfunction "PA10")
			(pintype "bidirectional+no_connect")
		)
		(pad "103" smd roundrect
			(at 10.6625 -6.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "unconnected-(U1-PA11-Pad103)")
			(pinfunction "PA11")
			(pintype "bidirectional+no_connect")
		)
		(pad "104" smd roundrect
			(at 10.6625 -6.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 148 "unconnected-(U1-PA12-Pad104)")
			(pinfunction "PA12")
			(pintype "bidirectional+no_connect")
		)
		(pad "105" smd roundrect
			(at 10.6625 -7.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "unconnected-(U1-PA13(JTMS-Pad105)")
			(pinfunction "PA13(JTMS")
			(pintype "bidirectional+no_connect")
		)
		(pad "106" smd roundrect
			(at 10.6625 -7.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "Net-(C27-Pad1)")
			(pinfunction "VCAP")
			(pintype "power_out")
		)
		(pad "107" smd roundrect
			(at 10.6625 -8.25)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "108" smd roundrect
			(at 10.6625 -8.75)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "109" smd roundrect
			(at 8.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "unconnected-(U1-PA14(JTCK-Pad109)")
			(pinfunction "PA14(JTCK")
			(pintype "bidirectional+no_connect")
		)
		(pad "110" smd roundrect
			(at 8.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "unconnected-(U1-PA15(JTDI)-Pad110)")
			(pinfunction "PA15(JTDI)")
			(pintype "bidirectional+no_connect")
		)
		(pad "111" smd roundrect
			(at 7.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 169 "unconnected-(U1-PC10-Pad111)")
			(pinfunction "PC10")
			(pintype "bidirectional")
		)
		(pad "112" smd roundrect
			(at 7.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 168 "unconnected-(U1-PC11-Pad112)")
			(pinfunction "PC11")
			(pintype "bidirectional")
		)
		(pad "113" smd roundrect
			(at 6.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "unconnected-(U1-PC12-Pad113)")
			(pinfunction "PC12")
			(pintype "bidirectional+no_connect")
		)
		(pad "114" smd roundrect
			(at 6.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "unconnected-(U1-PD0-Pad114)")
			(pinfunction "PD0")
			(pintype "bidirectional+no_connect")
		)
		(pad "115" smd roundrect
			(at 5.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "unconnected-(U1-PD1-Pad115)")
			(pinfunction "PD1")
			(pintype "bidirectional+no_connect")
		)
		(pad "116" smd roundrect
			(at 5.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "unconnected-(U1-PD2-Pad116)")
			(pinfunction "PD2")
			(pintype "bidirectional+no_connect")
		)
		(pad "117" smd roundrect
			(at 4.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "unconnected-(U1-PD3-Pad117)")
			(pinfunction "PD3")
			(pintype "bidirectional+no_connect")
		)
		(pad "118" smd roundrect
			(at 4.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "unconnected-(U1-PD4-Pad118)")
			(pinfunction "PD4")
			(pintype "bidirectional+no_connect")
		)
		(pad "119" smd roundrect
			(at 3.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "unconnected-(U1-PD5-Pad119)")
			(pinfunction "PD5")
			(pintype "bidirectional+no_connect")
		)
		(pad "120" smd roundrect
			(at 3.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "121" smd roundrect
			(at 2.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "122" smd roundrect
			(at 2.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 92 "unconnected-(U1-PD6-Pad122)")
			(pinfunction "PD6")
			(pintype "bidirectional+no_connect")
		)
		(pad "123" smd roundrect
			(at 1.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(U1-PD7-Pad123)")
			(pinfunction "PD7")
			(pintype "bidirectional+no_connect")
		)
		(pad "124" smd roundrect
			(at 1.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "unconnected-(U1-PG9-Pad124)")
			(pinfunction "PG9")
			(pintype "bidirectional+no_connect")
		)
		(pad "125" smd roundrect
			(at 0.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "unconnected-(U1-PG10-Pad125)")
			(pinfunction "PG10")
			(pintype "bidirectional+no_connect")
		)
		(pad "126" smd roundrect
			(at 0.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U1-PG11-Pad126)")
			(pinfunction "PG11")
			(pintype "bidirectional+no_connect")
		)
		(pad "127" smd roundrect
			(at -0.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 120 "unconnected-(U1-PG12-Pad127)")
			(pinfunction "PG12")
			(pintype "bidirectional+no_connect")
		)
		(pad "128" smd roundrect
			(at -0.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "unconnected-(U1-PG13-Pad128)")
			(pinfunction "PG13")
			(pintype "bidirectional+no_connect")
		)
		(pad "129" smd roundrect
			(at -1.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "unconnected-(U1-PG14-Pad129)")
			(pinfunction "PG14")
			(pintype "bidirectional+no_connect")
		)
		(pad "130" smd roundrect
			(at -1.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "131" smd roundrect
			(at -2.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "132" smd roundrect
			(at -2.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "unconnected-(U1-PG15-Pad132)")
			(pinfunction "PG15")
			(pintype "bidirectional+no_connect")
		)
		(pad "133" smd roundrect
			(at -3.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "unconnected-(U1-PB3(JTDO-Pad133)")
			(pinfunction "PB3(JTDO")
			(pintype "bidirectional+no_connect")
		)
		(pad "134" smd roundrect
			(at -3.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "unconnected-(U1-PB4(NJTRST)-Pad134)")
			(pinfunction "PB4(NJTRST)")
			(pintype "bidirectional+no_connect")
		)
		(pad "135" smd roundrect
			(at -4.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "unconnected-(U1-PB5-Pad135)")
			(pinfunction "PB5")
			(pintype "bidirectional+no_connect")
		)
		(pad "136" smd roundrect
			(at -4.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "unconnected-(U1-PB6-Pad136)")
			(pinfunction "PB6")
			(pintype "bidirectional+no_connect")
		)
		(pad "137" smd roundrect
			(at -5.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U1-PB7-Pad137)")
			(pinfunction "PB7")
			(pintype "bidirectional+no_connect")
		)
		(pad "138" smd roundrect
			(at -5.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "unconnected-(U1-BOOT0-Pad138)")
			(pinfunction "BOOT0")
			(pintype "input+no_connect")
		)
		(pad "139" smd roundrect
			(at -6.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "unconnected-(U1-PB8-Pad139)")
			(pinfunction "PB8")
			(pintype "bidirectional+no_connect")
		)
		(pad "140" smd roundrect
			(at -6.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 114 "unconnected-(U1-PB9-Pad140)")
			(pinfunction "PB9")
			(pintype "bidirectional+no_connect")
		)
		(pad "141" smd roundrect
			(at -7.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "unconnected-(U1-PE0-Pad141)")
			(pinfunction "PE0")
			(pintype "bidirectional+no_connect")
		)
		(pad "142" smd roundrect
			(at -7.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "unconnected-(U1-PE1-Pad142)")
			(pinfunction "PE1")
			(pintype "bidirectional+no_connect")
		)
		(pad "143" smd roundrect
			(at -8.25 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "unconnected-(U1-PDR_ON-Pad143)")
			(pinfunction "PDR_ON")
			(pintype "input+no_connect")
		)
		(pad "144" smd roundrect
			(at -8.75 -10.6625)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-144_20x20mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 258.2125 132.25 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C31"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 151 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 76.25 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D9"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0.885 0.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 2 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 67.25 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D12"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 23 "Net-(D12-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 147.475 47)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U7"
			(at 0 -5.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC126D"
			(at 0 5.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hc126.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quadruple Buffers with 3-State Outputs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC14 SOIC14-M SOIC14-L")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "RXEN")
			(pinfunction "1OE")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J1-Pin_2)")
			(pinfunction "1A")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 173 "RXD")
			(pinfunction "1Y")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "TXEN")
			(pinfunction "2OE")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 171 "TXD")
			(pinfunction "2A")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J1-Pin_2)")
			(pinfunction "2Y")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "unconnected-(U7-3Y-Pad8)")
			(pinfunction "3Y")
			(pintype "tri_state+no_connect")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 164 "unconnected-(U7-3A-Pad9)")
			(pinfunction "3A")
			(pintype "input+no_connect")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "unconnected-(U7-3OE-Pad10)")
			(pinfunction "3OE")
			(pintype "input+no_connect")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "unconnected-(U7-4Y-Pad11)")
			(pinfunction "4Y")
			(pintype "tri_state+no_connect")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "unconnected-(U7-4A-Pad12)")
			(pinfunction "4A")
			(pintype "input+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "unconnected-(U7-4OE-Pad13)")
			(pinfunction "4OE")
			(pintype "input+no_connect")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_SPT:PhoenixContact_SPT_1.5_2-H-3.5_1x02_P3.5mm_Horizontal"
		(layer "F.Cu")
		(at 208.5 24.7 180)
		(descr "Connector Phoenix Contact, SPT 1.5/2-H-3.5 Terminal Block, 1990737 (https://www.phoenixcontact.com/online/portal/gb/?uri=pxc-oc-itemdetail:pid=1990737), generated with kicad-footprint-generator")
		(tags "Connector Phoenix Contact SPT 1.5/2-H-3.5 1990737")
		(property "Reference" "J2"
			(at 2.9 -3.73 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 2.9 13.27 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Phoenix_SPT:PhoenixContact_SPT_1.5_2-H-3.5_1x02_P3.5mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.9 -1.83 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.8 3.3)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 31 "+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "1" thru_hole roundrect
			(at 0 8.2 180)
			(size 1.8 3.3)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 31 "+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.5 0 180)
			(size 1.8 3.3)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.5 8.2 180)
			(size 1.8 3.3)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Phoenix_SPT.3dshapes/PhoenixContact_SPT_1.5_2-H-3.5_1x02_P3.5mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 251.13 14.97 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 31 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.25 40.25 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 37 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(J1-Pin_2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 254.13 30.97 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "7.5k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(C4-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 70)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(D11-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 26 "Net-(J5-Pin_5)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 249.25 70.15 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 25 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Converter_DCDC:Converter_DCDC_Murata_MEE1SxxxxSC_THT"
		(layer "F.Cu")
		(at 144.4075 26.23)
		(descr "https://power.murata.com/pub/data/power/ncl/kdc_mee1.pdf")
		(tags "murata dc-dc transformer")
		(property "Reference" "PS1"
			(at 0.5 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MEE1S1205SC (FISM-1769205241)"
			(at 1.5 11 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_Murata_MEE1SxxxxSC_THT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://power.murata.com/pub/data/power/ncl/kdc_mee1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1W, 1000 VDC isolated DC/DC converter, 12V input, 5V output, SIP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Converter*DCDC*Murata*MEE1SxxxxSC*THT*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.794 3.556 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.75 2.25)
			(drill 1.075)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 179 "Net-(PS1--Vin)")
			(pinfunction "-Vin")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.75 2.25)
			(drill 1.075)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 180 "Net-(PS1-+Vin)")
			(pinfunction "+Vin")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.75 2.25)
			(drill 1.075)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND")
			(pinfunction "-Vout")
			(pintype "power_out")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.75 2.25)
			(drill 1.075)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "+5V")
			(pinfunction "+Vout")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_MEE1SxxxxSC_THT.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 252 64)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 22 "Net-(D13-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 21 "Net-(J5-Pin_7)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 258.12 20.97 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 10 "3.3V{slash}2A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "F.Cu")
		(at 224.75 60.5 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D16"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "TVS"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1071428571)
			(net 42 "RX")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 248.13 14.9325 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 31 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 245.13 22.9325 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C32"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 34 "Net-(U4-BS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.212766)
			(net 29 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
		(layer "F.Cu")
		(at 245.13 29.295 -90)
		(descr "Inductor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L1"
			(at 0 -1 90)
			(layer "F.SilkS")
		)
		(property "Value" "6.8uH"
			(at 0 1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_01005_0402Metric_Pad0.57x0.30mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.62 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.3625 0 270)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.3625 0 270)
			(size 0.41 0.27)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3375 0 270)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(D1-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3375 0 270)
			(size 0.575 0.3)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "3.3V{slash}2A")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_01005_0402Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 218 68)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C23"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 214 71 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 204.5 81.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C25"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 44 "Net-(U1-VREF+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 280 137.75 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C29"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 12 "Net-(D4-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 212.5 62)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C24"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 141.25 32.5 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C36"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 37 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 212 85.9 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0.5 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 226.5 75 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 211 76 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 278 133.5 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C30"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 16 "Net-(D5-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "B.Cu")
		(at 278 137.035 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D4"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "TVS"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1071428571)
			(net 12 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 229 80.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C21"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 152.25 27 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C35"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 180 "Net-(PS1-+Vin)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 179 "Net-(PS1--Vin)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 229 68.9625 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 204.5 87.0375 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 218.5 86 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 152.25 32 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C34"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "470pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 180 "Net-(PS1-+Vin)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 207 81.4625 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C26"
			(at -0.5 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.5 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 44 "Net-(U1-VREF+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 228 86)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 46 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 211.5 71 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 229 75 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 211.2 82.9625 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 253.25 133.25 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "270"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 17 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 18 "Net-(U3-CBUS0)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 232.5 70.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C28"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 46 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 223.5 86 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 207 87.0375 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "B.Cu")
		(at 280.75 132.25 -90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D3"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "TVS"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 270)
			(size 0.93 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1071428571)
			(net 13 "+3.3V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 270)
			(size 0.3 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 229.9625 89.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C19"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 212.5 64.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "B.Cu")
		(at 276 134.25 90)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D5"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "TVS"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0 90)
			(size 0.93 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1071428571)
			(net 16 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0 90)
			(size 0.3 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
		(layer "B.Cu")
		(at 120.785 17)
		(descr "Diode SMD DSN1608, 1.6 x 0.8 x 0.29 mm, https://assets.nexperia.com/documents/package-information/SOD964.pdf")
		(tags "diode SOD964 SOD-964")
		(property "Reference" "D6"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "TVS"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Diode_SMD:Nexperia_DSN1608-2_1.6x0.8mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PTVS5V0Z1USK.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "5V, 1200W TVS unidirectional diode, DSN1608-2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*DSN1608?2*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.285 0)
			(size 0.93 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.1071428571)
			(net 31 "+12V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.6 0)
			(size 0.3 0.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/Nexperia_DSN1608-2_1.6x0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 158.75 29.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C33"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 31 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 222.9625 68)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C22"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "MCU.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 13 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.212766)
			(net 8 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
)
