CE 470: Design of Metal Structures – Prof. Dr. A. Varma


Solutions to Homework 12:
Problem No. 1
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Note that (bMp=611 kip-ft
Problem No. 2
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Problem No. 3
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Sum Moments at A equal zero
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Note that (bMp = 1560 kip-ft (ok)




























PAGE  
1

