CE 470: Design of Steel Structures – Prof. Varma
CHAPTER 4. COMPRESSION MEMBER DESIGN

4.1 INTRODUCTORY CONCEPTS
· Compression Members:  Structural elements that are subjected to axial compressive forces only are called columns. Columns are subjected to axial loads throughu the centroid. 
· Stress: The stress in the column cross-section can be calculated as 

						(2.1)
where, f is assumed to be uniform over the entire cross-section. 
· This ideal state is never reached. The stress-state will be non-uniform due to:
· Accidental eccentricity of loading with respect to the centroid
· Member out-of –straightness (crookedness), or
· Residual stresses in the member cross-section due to fabrication processes.
· Accidental eccentricity and member out-of-straightness can cause bending moments in the member. However, these are secondary and are usually ignored.
· Bending moments cannot be neglected if they are acting on the member. Members with axial compression and bending moment are called beam-columns.

4.2 COLUMN BUCKLING
· Consider a long slender compression member. If an axial load P is applied and increased slowly, it will ultimately reach a value Pcr that will cause buckling of the column (Figure 1). Pcr is called the critical buckling load of the column.


What is buckling?
Buckling occurs when a straight column subjected to axial compression suddenly undergoes bending as shown in the Figure 1(b). Buckling is identified as a failure limit-state for columns. 


Figure 1. Buckling of axially loaded compression members

· The critical buckling load Pcr for columns is theoretically given by Equation (4.1)

Pcr = 					(4.1)
where, I = moment of inertia about axis of buckling
	     K = effective length factor based on end boundary conditions
· Effective length factors are given on page 16.1-511240 (Table C-A-7.1) of the AISC manual.

· In examples, homeworks, and exams please state clearly whether you are using the theoretical value of K or the recommended design values.


EXAMPLE 4.1 Determine the buckling strength of a W 12 x 50 column. Its length is 20 ft. For major axis buckling, it is pinned at both ends. For minor buckling, is it pinned at one end and fixed at the other end.
Solution
Step I. Visualize the problem
  	








Figure 2. (a) Cross-section; (b) major-axis buckling; (c) minor-axis buckling


· For the W12 x 50 (or any wide flange section), x is the major axis and y is the minor axis. Major axis means axis about which it has greater moment of inertia (Ix > Iy)
              
Figure 3. (a) Major axis buckling; (b) minor axis buckling


Step II. Determine the effective lengths
· According to Table C-A-7.1C2.2 of the AISC Manual (see page 16.1 - 511240):
· For pin-pin end conditions about the major axis 
Kx = 1.0 (theoretical value); and Kx = 1.0 (recommended design value)
· For pin-fix end conditions about the minor axis
Ky = 0.7 (theoretical value); and Ky = 0.8 (recommended design value)
· According to the problem statement, the unsupported length for buckling about the major (x) axis = Lx = 20 ft.
· The unsupported length for buckling about the minor (y) axis = Lx = 20 ft. 
· Effective length for major (x) axis buckling = Kx Lx = 1.0 x 20 = 20 ft. = 240 in. 
· Effective length for minor (y) axis buckling = Ky Ly = 0.8 x 20 = 16 ft. = 192 in.
Step III. Determine the relevant section properties
· For W12 x 50: elastic modulus = E = 29000 ksi (constant for all steels)
· For W12 x 50: 	Ix = 391 in4. 	Iy = 56.3 in4  (see pages 1-26 and 1-275 of the AISC manual)
Step IV. Calculate the buckling strength
· 

Critical load for buckling about x - axis = Pcr-x =  = 
Pcr-x = 1942.9 kips
· 

Critical load for buckling about y-axis = Pcr-y = =
Pcr-y = 437.12 kips
· Buckling strength of the column = smaller (Pcr-x, Pcr-y) = Pcr = 437.12 kips 
Minor (y) axis buckling governs. 

· Notes:
· Minor axis buckling usually governs for all doubly symmetric cross-sections. However, for some cases, major (x) axis buckling can govern.
· Note that the steel yield stress was irrelevant for calculating this buckling strength.

4.3 INELASTIC COLUMN BUCKLING

· Let us consider the previous example. According to our calculations Pcr = 437 kips. This Pcr will cause a uniform stress f = Pcr/A in the cross-section
· For W12 x 50, A = 14.6 in2. Therefore, for Pcr = 437 kips; f = 30 ksi
The calculated value of f is within the elastic range for a 50 ksi yield stress material.
· 
However, if the unsupported length was only 10 ft., Pcr =would be calculated as 1748119 kips, and f = 76.6119.73 ksi. 
· This value of f is ridiculous because the material will yield at 50 ksi and never develop f = 119.7376.6 ksi. The member would yield before buckling. 
· Equation (4.1) is valid only when the material everywhere in the cross-section is in the elastic region. If the material goes inelastic then Equation (4.1) becomes useless and cannot be used.
· What happens in the inelastic range?
Several other problems appear in the inelastic range. 
· The member out-of-straightness has a significant influence on the buckling strength in the inelastic region. It must be accounted for.
· The residual stresses in the member due to the fabrication process causes yielding in the cross-section much before the uniform stress f reaches the yield stress Fy. 
· The shape of the cross-section (W, C, etc.) also influences the buckling strength. 
· In the inelastic range, the steel material can undergo strain hardening.

All of these are very advanced concepts and beyond the scope of CE470. You are welcome to CE579 to develop a better understanding of these issues. 

· So, what should we do? We will directly look at the AISC Specifications for the strength of compression members, i.e., Chapter E (page 16.1-31 2 of the AISC manual).

4.4 AISC SPECIFICATIONS FOR COLUMN STRENGTH
· The AISC specifications for column design are based on several years of research. 
· These specifications account for the elastic and inelastic buckling of columns including all issues (member crookedness, residual stresses, accidental eccentricity etc.) mentioned above.
· The specification presented here (AISC Spec E3) will work for all doubly symmetric cross-sections and channel sections.
· The design strength of columns for the flexural buckling limit state is equal to cPn
Where,	 c = 0.9		(Resistance factor for compression members)
			Pn = Ag Fcr								(4.2)
· 

When 	(or )
· 
Fcr =  Fy  					(4.3)
· 


When 	(or )

				Fcr = 					(4.4)

Where, Fe = 								(4.5)
	Ag = gross member area;			K = effective length factor
	L = unbraced length of the member; 		r = correspondinggoverning radius of gyration

           
· 
Note that the original Euler buckling equation is Pcr = 

 
· 
Note that the AISC equation for  is Fcr = 0.877Fe
· The 0.877 factor tries to account for initial crookedness.
· For a given column section:
· Calculate I, Ag, r 
· Determine effective length K L based on end boundary conditions. 
· 
Calculate Fe, 0.44Fy/Fe , or 
· 
If (KL/r) greater than , elastic buckling occurs and use Equation (4.4)
· 
If (KL/r) is less than or equal to , inelastic buckling occurs and use Equation (4.3)
· Note that the column can develop its yield strength Fy as (KL/r) approaches zero. 

4.5 COLUMN STRENGTH 
· In order to simplify calculations, the AISC specification includes Tables. 
· Table 4-22 on pages 4-322 to 4-32618 shows KL/r vs. cFcr for various steels.
· You can calculate KL/r for the column, then read the value of cFcr from this table
· The column strength will be equal to cFcr x Ag

EXAMPLE 4.2 Calculate the design strength of W14 x 74 with length of 20 ft. and pinned ends. A36 steel is used.
Solution
· Step I. Calculate the effective length and slenderness ratio for the problem
Kx = Ky = 1.0
Lx = Ly = 240 in.
Major axis slenderness ratio = KxLx/rx = 240/6.04 = 39.735
Minor axis slenderness ratio = KyLy/ry = 240/2.48 = 96.77
· Step II. Calculate the elastic critical buckling stress
The governing slenderness ratio is the larger of (KxLx/rx, KyLy/ry)

= 30.56 ksi
Check the limits


		( ) or ()




Since Since;	Therefore, Fcr =  Fy 
Therefore, Fcr = 21.99 ksi
Design column strength = cPn = 0.9 (Ag Fcr) = 0.985 (21.8 in2 x 21.99 ksi) = 431.4 kips
Design strength of column = 431 kips
· Check calculated values with Table 4-22. For KL/r = 97, cFcr = 19.7 ksi
· 
4.6 LOCAL BUCKLING LIMIT STATE
· The AISC specifications for column strength assume that column buckling is the governing limit state. However, if the column section is made of thin (slender) plate elements, then failure can occur due to local buckling of the flanges or the webs. 

Figure 4. Local buckling of columns
· If local buckling of the individual plate elements occurs, then the column may not be able to develop its buckling strength. 
· Therefore, the local buckling limit state must be prevented from controlling the column strength.
· Local buckling depends on the slenderness (width-to-thickness b/t ratio) of the plate element and the yield stress (Fy) of the material. 
· Each plate element must be stocky enough, i.e., have a b/t ratio that prevents local buckling from governing the column strength. 
· The AISC specification B4.1 (Page 16.1-14) provides the slenderness (b/t) limits that the individual plate elements must satisfy so that local buckling does not control. 
· For compression, Tthe AISC specification provides two slenderness limits (p and r) for the local buckling of plate elements. 
[bookmark: _GoBack]
 Figure 5. Local buckling behavior and classification of plate elements
· If the slenderness ratio (b/t) of the plate element is greater than r then it is slender. It will locally buckle in the elastic range before reaching Fy
· If the slenderness ratio (b/t) of the plate element is less than r but greater than p, then it is non-slendercompact. It will not locally buckle immediately afterin elastic range before reaching Fy
· 
· If the slenderness ratio (b/t) of the plate element is less than f, then the element is compact. It will locally buckle much after reaching Fy
If all the plate elements of a cross-section are compact, then the section is compact.
If any one plate element is non-compact, then the cross-section is non-compact
· If any one plate element is slender, then the cross-section is slender.
· The slenderness limit s p and r for various plate elements with different boundary conditions are given in Table B4.1a on pages from  16.1-16 to 16.1-18 of the AISC Spec.
· Note that the slenderness limits (p and r) and the definition of plate slenderness (b/t) ratio depend upon the boundary conditions for the plate. 
· If the plate is supported along two edges parallel to the direction of compression force, then it is a stiffened element. For example, the webs of W shapes
· If the plate is supported along only one edge parallel to the direction of the compression force, then it is an unstiffened element, e.g. Ex., the flanges of W shapes.

· The local buckling limit state can be prevented from controlling the column strength by using sections that are nonslender.-compact
· If all the elements of the cross-section have calculated slenderness (b/t) ratio less than r, then the local buckling limit state will not control. 
· For the definitions of b/t and , p, r for various situations see Table B4.1a and Spec B4.15. 

EXAMPLE 4.3 Determine the local buckling slenderness limits and evaluate the W14 x 74 section used in Example 4.2. Does local buckling limit the column strength?
Solution
· Step I. Calculate the slenderness limits
See Table B4.1a on pages 16.1- – 16 to 16.1-18. 
· For the flanges of I-shape sections in pure compression


r = 0.56 x = 0.56 x  = 15.9
· For the webs of I-shapes section in pure compression


r = 1.49 x = 1.49 x = 42.3
· Step II. Calculate the slenderness ratios for the flanges and webs of W14 x 74
· For the flanges of I-shape member, b = bf/2 = flange width / 2  
Therefore, b/t = bf/2tf.					
For W 14 x 74, bf/2tf = 6.413				(See Page 1-243 in AISC)
· For the webs of I shaped member, b = h
h is the clear distance between flanges less the fillet / corner radius of each flange
For W14 x 74, h/tw = 25.424.17				(See Page 1-243 in AISC)
· Step III. Make the comparisons and comment
For the flanges, b/t < r. Therefore, the flange is nonslender-compact
For the webs, h/tw < r. Therefore the web is nonslender-compact
Therefore, the section is nonslender.-compact
Therefore, local buckling will not limit the column strength. 

4.7 COLUMN DESIGN
· The AISC manual has tables for column strength. See page 4-120 onwards. 
· For wide flange sections, the column buckling strength (cPn) is tabulated with respect to the effective length about the minor axis KyLy in Table 4-1.
· The table takes the KyLy value for a section, and internally calculates the KyLy/ry, and then calculates the tabulated column strength using either Equation E3-2 or E3-3 of the specification.
· If you want to use the Table 4-1 for calculating the column strength for buckling about the major axis, then do the following:
· 
Take the major axis KxLx value. Calculate an equivalent (KL)eq = 
· Use the calculated (KL)eq value to find (cPn) the column strength for buckling about the major axis from Table (4-1) 
· For example, consider a W14 x 74 column with KyLy = 20 ft. and KxLx = 25 ft. 
· Material has yield stress = 50 ksi (always in Table 4-1).
· See Table 4-1, for KyLy = 20 ft., cPn = 4954 kips (minor axis buckling strength)
· rx/ry for W14x74 = 2.44 from Table 4-1 (see page 4-164 of AISC).
· For KxLx = 25 ft., (KL)eq = 25/2.44 = 10.25 ft. 
· For (KL)eq = 10.25 ft., cPn = 774 819.5 kips (major axis buckling strength)
· If calculated value of (KL)eq < KyLy then minor axis buckling will govern.

EXAMPLE 4.4 Determine the design strength of an ASTM A992 W14 x 132 that is part of a braced frame. Assume that the physical length L = 30 ft., the ends are pinned and the column is braced at the ends only for the X-X axis and braced at the ends and mid-height for the Y-Y axis. 
Solution
· Step I. Calculate the effective lengths.
For W14 x 132: 	rx = 6.28 in;	ry = 3.76 in;	Ag =38.8 in2	
Kx = 1.0	and 	Ky = 1.0
Lx = 30 ft.	and	Ly = 15 ft.
KxLx = 30 ft.  and 	KyLy = 15 ft. 
· Step II. Determine the governing slenderness ratio
KxLx/rx = 30 x 12 in./6.28 in.= 57.32
KyLy/ry = 15 x 12 in./3.76 in. = 47.87
The larger slenderness ratio, therefore, buckling about the major axis will govern the column strength. 
· Step III. Calculate the column strength


KxLx = 30 ft.	Therefore, (KL)eq =  =  = 17.96 ft.
From Table 4-1,	for  (KL)eq = 18.0 ft.	 cPn = 1370 kips (design column strength)
· Step IV. Check the local buckling limits

For the flanges, bf/2tf = 7.145	< 	r = 0.56 x = 13.5	

For the web, h/tw = 17.75.5		< 	r = 1.49 x = 35.9
Therefore, the section is nonslender-compact. OK. 

EXAMPLE 4.5 A compression member is subjected to service loads of 165 kips dead load and 535 kips of live load. The member is 26 ft. long and pinned at each end. Use A992 (50 ksi) steel and select a W shape
Solution
· Calculate the factored design load Pu
Pu = 1.2 PD + 1.6 PL = 1.2 x 165 + 1.6 x 535 = 1054 kips

· Select a W shape from the AISC manual Tables
For KyLy = 26 ft. and required strength = 1054 kips 
· Select W14 x 145 from page 4-153. It has cPn = 1230 kips 
· Select W12 x 170 from page 4-186. It has cPn = 1130 kips
· No W10 will work. See Page 4-2119
· W14 x 145 is the lightest.

· Note that column sections are usually W12 or W14. Usually sections bigger than W14 are usually not used as columns. 


4.8 EFFECTIVE LENGTH OF COLUMNS IN FRAMES
· So far, we have looked at the buckling strength of individual columns. These columns had various boundary conditions at the ends, but they were not connected to other members with moment (fix) connections. 
· The effective length factor K for the buckling of an individual column can be obtained for the appropriate end conditions from Table C-A-7.1C2.2 of the AISC Manual .
· However, when these individual columns are part of a frame, their ends are connected to other members (beams etc.). 
· Their effective length factor K will depend on the restraint offered by the other members connected at the ends. 
· Therefore, the effective length factor K will depend on the relative rigidity (stiffness) of the members connected at the ends.
The effective length factor for columns in frames must be calculated as follows:
· First, you have to determine whether the column is part of a braced frame or an unbraced (moment resisting) frame. 
· If the column is part of a braced frame then its effective length factor 0.5 < K ≤ 1
· If the column is part of an unbraced frame then 1 < K ≤ ∞
· Then, you have to determine the relative rigidity factor G for both ends of the column
· G is defined as the ratio of the summation of the rigidity (EI/L) of all columns coming together at an end to the summation of the rigidity (EI/L) of all beams coming together at the same end. 
· 
G = 		- It must be calculated for both ends of the column.
· Then, you can determine the effective length factor K for the column using the calculated value of G at both ends, i.e., GA and GB and the appropriate alignment chart
· There are two alignment charts provided by the AISC manual, 
· One is for columns in braced (sidesway inhibited) frames. See Figure C-A-7.1C2.3 on page 16.1-512241 of the AISC manual. 0 < K ≤ 1
· The second is for columns in unbraced (sidesway uninhibited) frames. See Figure C-A-7.2 C2.4 on page 16.1-513242 of the AISC manual. 1 < K ≤ ∞
· The procedure for calculating G is the same for both cases. 

EXAMPLE 4.6 Calculate the effective length factor for the W12 x 53 column AB of the frame shown below. Assume that the column is oriented in such a way that major axis bending occurs in the plane of the frame. Assume that the columns are braced at each story level for out-of-plane buckling. Assume that the same column section is used for the stories above and below. 

Step I. Identify the frame type and calculate Lx, Ly, Kx, and Ky if possible.
· It is an unbraced (sidesway uninhibited) frame. 
· Lx = Ly = 12 ft.
· Ky = 1.0
· Kx depends on boundary conditions, which involve restraints due to beams and columns connected to the ends of column AB.
· Need to calculate Kx using alignment charts.

Step II - Calculate Kx
· Ixx of W 12 x 53 = 425 in4			Ixx of W14x68 = 72253
· 

· 

· Using GA and GB: Kx = 1.3 			- from Alignment Chart on Page 16.1-5133-6

Step III – Design strength of the column 
· KyLy = 1.0 x 12 = 12 ft.
· Kx Lx = 1.3 x 12 = 15.6 ft.
· rx / ry for W12x53 = 2.11
· (KL)eq = 15.6 / 2.11 = 7.4 ft.
· KyLy > (KL)eq 
· Therefore, y-axis buckling governs. Therefore cPn = 5497 kips

4.8.1 Inelastic Stiffness Reduction Factor – Modification
· This concept for calculating the effective length of columns in frames was widely accepted for many years. 
· Over the past few years, a lot of modifications have been proposed to this method due to its several assumptions and limitation. Most of these modifications have not yet been accepted in to the AISC provisions. Some of these modifications have been accepted into AISC provisions as Adjustments (Comm. 7.2 Pages 16.1-513 and 16.1-514).
· One of the accepted modifications is the inelastic stiffness reduction factor. As presented earlier, G is a measure of the relative flexural rigidity of the columns (EIc/Lc) with respect to the beams (EIb/Lb)
· However, if column buckling were to occur in the inelastic range (c < 1.5), then the flexural rigidity of the column will be reduced because Ic will be the moment of inertia of only the elastic core of the entire cross-section. See figure below

· The beams will have greater flexural rigidity when compared with the reduced rigidity (EIc) of the inelastic columns. As a result, the beams will be able to restrain the columns better, which is good for column design. 
· This effect is incorporated in to the AISC column design method through the use of Table 4-21 given on page 4-32117 of the AISC manual. 
· Table 4-21 gives the stiffness reduction factor () as a function of the yield stress Fy and the stress Pu/Ag in the column, where Pu is factored design load (analysis)

EXAMPLE 4.7 Calculate the effective length factor for a W10 x 60 column AB made from 50 ksi steel in the unbraced frame shown below. Column AB has a design factor load Pu = 450 kips. The columns are oriented such that major axis bending occurs in the plane of the frame. The columns are braced continuously along the length for out-of-plane buckling. Assume that the same column section is used for the story above


Solution
Step I. Identify the frame type and calculate Lx, Ly, Kx, and Ky if possible.
· It is an unbraced (sidesway uninhibited) frame. 
· Ly = 0 ft.
· Ky has no meaning because out-of-plane buckling is not possible.
· Kx depends on boundary conditions, which involve restraints due to beams and columns connected to the ends of column AB.
· Need to calculate Kx using alignment charts.

Step II (a)  - Calculate Kx 
· Ixx of W 14 x 74 = 796 in4				Ixx of W 10 x 60 = 341 in4
· 

· 
					- for pin support, see note on Page 16.1-513241

· Using GA and GB: Kx = 1.8 		- from Alignment Chart on Page 16.1-513242

· Note, Kx is greater than 1.0 because it is an unbraced frame. 

Step II (b) - Calculate Kx– inelastic using stiffness reduction factor method
· Reduction in the flexural rigidity of the column due to residual stress effects
· First calculate, Pu / Ag = 450 / 17.76 = 25.4257 ksi
· Then go to Table 4-21 on page 4-32117 of the manual, and read the value of stiffness reduction factor for Fy = 50 ksi and Pu/Ag = 25.4257 ksi.
· Stiffness reduction factor =  = 0.999878
· GA-inelastic =  x GA = 0.87999 8 x 0.609 = 0.6084535

· GB = 10				- for pin support, see note on Page 16.1-513241

· Using GA-inelastic and GB, Kx-inelastic = 1.875 		- alignment chart on Page 16.1-513242

· Note: You can combine Steps II (a) and (b) to calculate the Kx-inelastic directly. You don’t need to calculate elastic Kx first. It was done here for demonstration purposes.
· Note that Kx-inelastic< Kx. This is in agreement with the fact that the beams offer better resistance to the inelastic column AB because it has reduced flexural rigidity.

Step III – Design strength of the column 
· KxLx = 1.875 x 15 = 26.2527 ft.
· rx / ry for W10x60 = 1.71			- from Table 4-1, see page 4-2119
· (KL)eq = 26.25/1.71 = 15.835 ft.
· cPn for X-axis buckling = 535.245 kips 		- from Table 4-1, see page 4-2119

· Section slightly over-designed for Pu = 450 kips. 

Column design strength = cPn = 535.245 kips


EXAMPLE 4.8: 

· Design Column AB of the frame shown below for a design load of 500 kips. 
· Assume that the column is oriented in such a way that major axis bending occurs in the plane of the frame. 
· Assume that the columns are braced at each story level for out-of-plane buckling.
· Assume that the same column section is used for the stories above and below. 



Step I - Determine the design load and assume the steel material.
· Design Load = Pu = 500 kips
· Steel yield stress = 50 ksi (A992 material)

Step II. Identify the frame type and calculate Lx, Ly, Kx, and Ky if possible.
· It is an unbraced (sidesway uninhibited) frame. 
· Lx = Ly = 12 ft.
· Ky = 1.0
· Kx depends on boundary conditions, which involve restraints due to beams and columns connected to the ends of column AB.
· Need to calculate Kx using alignment charts.
· Need to select a section to calculate Kx

Step III - Select a column section
· Assume minor axis buckling governs.
· Ky Ly = 12 ft.
· See Column Tables in AISC-LRFD manual 
Select section W12x53
· cPn for y-axis buckling = 5497 kips

Step IV - Calculate Kx-inelastic
· Ixx of W 12 x 53 =425 in4			Ixx of W14x68 = 75223 in4
· Account for the reduced flexural rigidity of the column due to residual stress effects
· Pu/Ag = 500 / 15.6 = 32.05 ksi
· Stiffness reduction factor =  = 0.92266
· 

· 

· Using GA and GB: Kx-inelastic = 1.28 			- from Alignment Chart

Step V - Check the selected section for X-axis buckling
· Kx Lx = 1.28 x 12 = 15.364.4 ft.
· rx / ry for W12x53 = 2.11
· Calculate (KL)eq to determine strength (cPn) for X-axis buckling 
(KL)eq = 15.364.4 / 2.11 = 7.2806.825 ft.
· From the column design tables, cPn for X-axis buckling = 6441.24 kips 

Step VI. Check the local buckling limits

For the flanges, bf/2tf = 8.7069	< 	r = 0.56 x = 13.5	

For the web, h/tw = 26.818.1		< 	r = 1.49 x = 35.9
	Therefore, the section is nonslender-compact. OK, local buckling is not a problem

Step VII - Summarize the solution

	Lx = Ly = 12 ft.  		Ky = 1.0		

	Kx = 1.28 (inelastic buckling - sway frame-alignment chart method)

	cPn for Y-axis buckling = 51849 kips

	cPn for X-axis buckling = 641.244 kips

	Y-axis buckling governs the design.

	Selected Section is W12 x 53 made from 50 ksi steel.





EXAMPLE 4.9
· Design Column AB of the frame shown below for a design load of 450 kips. 
· Assume that the column is oriented in such a way that major axis bending occurs in the plane of the frame. 
· Assume that the columns are braced continuously along the length for out-of-plane buckling.
· Assume that the same column section is used for the story above.

Step I - Determine the design load and assume the steel material.
· Design Load = Pu = 450 kips
· Steel yield stress = 50 ksi

Step II. Identify the frame type and calculate Lx, Ly, Kx, and Ky if possible.
· It is an unbraced (sidesway uninhibited) frame. 
· Ly = 0 ft.
· Ky has no meaning because out-of-plane buckling is not possible.
· Kx depends on boundary conditions, which involve restraints due to beams and columns connected to the ends of column AB.
· Need to calculate Kx using alignment charts.
· Need to select a section to calculate Kx


Step III. Select a section
· There is no help from the minor axis to select a section
· Need to assume Kx to select a section.
See Figure below:


· The best case scenario for Kx is when the beams connected at joint A have infinite flexural stiffness (rigid). In that case Kx = 2.0 from Table C-A-7.1C2.1 
· Actually, the beams don't have infinite flexural stiffness. Therefore, calculated Kx should be greater than 2.0. 
· To select a section, assume Kx = 2.0
· KxLx = 2.0 x 15.0 ft. = 30.0 ft.
· Need to be able to calculate (KL)eq to be able to use the column design tables to select a section. Therefore, need to assume a value of rx/ry to select a section.
· See the W10 column tables on pages 4-21 and 4-226. 
· Assume rx/ry = 1.71, which is valid for W10 x 49 to W10 x 68. 
· (KL)eq = 30.0/1.71 = 17.54 ft.
· Obviously from the Tables, for (KL)eq = 17.5 ft., W10 x 60 is the first section that will have cPn > 450 kips
· Select W10x60 with cPn = 488.557.7 kips for (KL)eq = 17.5 ft. 

Step IV - Calculate Kx-inelastic using selected section
· Ixx of W 14 x 74 = 7956 in4			Ixx of W 10 x 60 = 341 in4
· Account for the reduced flexural rigidity of the column due to residual stress effects
· Pu/Ag = 450 / 17.76 = 25.4257 ksi
· Stiffness reduction factor =  = 0.999863
· 

· 
						- for pin support
· Using GA and GB: Kx-inelastic = 1.875		- from Alignment Chart on Page 16.1-5133-6
· 
Calculated value of Kx-inelastic is less than 2.0 (the assumed value) because GB was assumed to be equal to 10 instead of 

Step V - Check the selected section for X-axis buckling
· Kx Lx = 1.875 x 15 = 276.25 ft.
· rx / ry for W10x60 = 1.71
· (KL)eq = 276.25/1.71 = 15.8035 ft. 
· (cPn) for X-axis buckling = 535.245.5 kips
· Section slightly over-designed for Pu = 450 kips. 
· W10 x 54 will probably be adequate, Student should check by calculating Kx inelastic and cPn for that section. 

Step VI. Check the local buckling limits

For the flanges, bf/2tf = 7.431	< 	r = 0.56 x = 13.5	

For the web, h/tw = 17.868.7		< 	r = 1.49 x = 35.9
	Therefore, the section is nonslender-compact. OK, local buckling is not a problem

· 
Step VII - Summarize the solution

	Ly = 0 ft.  		Ky = no buckling		

	Kx = 1.875 (inelastic buckling - sway frame - alignment chart method)

	cPn for X-axis buckling = 535.245 kips

	X-axis buckling governs the design.

	Selected section is W10 x 60 
(W10 x 54 will probably be adequate).
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