CE 470: Design of Steel Structures –  Dr. Amit Varma
1.0 INTRODUCTION TO STRUCTURAL ENGINEERING 

1.1 GENERAL INTRODUCTION
Structural design is a systematic and iterative process that involves:
1) Identification of intended use and occupancy of a structure – by owner
2) Development of architectural plans and layout – by architect
3) Identification of structural framework – by engineer
4) Estimation of structural loads depending on use and occupancy 
5) Analysis of the structure to determine member and connection design forces 
6) Design of structural members and connections
7) Verification of design 
8) Fabrication & Erection – by steel fabricator and contractor
9) Inspection and Approval – by state building official

Ideally, the owner and the architect, the architect and the engineer, and the engineer and the fabricator/contractor will collaborate and interact on a regular basis to conceive, develop, design, and build the structure in an efficient manner. The primary responsibilities of all these players are as follows:
· Owner - primary responsibility is deciding the use and occupancy, and approving the architectural plans of the building. 
· Architect - primary responsibility is ensuring that the architectural plan of the building interior is appropriate for the intended use and the overall building is aesthetically pleasing.
· Engineer – primary responsibility is ensuring the safety and serviceability of the structure, i.e., designing the building to carry the loads safely and ___________.
· Fabricator – primary responsibility is ensuring that the designed members and connections are fabricated economically in the shop or field as required. 
· Contractor/Erector - primary responsibility is ensuring that the members and connections are economically assembled in the field to build the structure.
· State Building Official – primary responsibility is ensuring that the built structure satisfies the appropriate building codes accepted by the Govt.

1.2 STRUCTURAL DESIGN 
· Conceptually, from an engineering standpoint, the parameters that can be varied (somewhat) are: (1) the material of construction, and (2) the structural framing plan. 
· The choices for material include: (a) steel, (b) reinforced concrete, and (c) steel-concrete composite construction. 
· The choices for structural framing plan include moment resisting frames, braced frames, dual frames, shear wall frames, and so on. The engineer can also innovate a new structural framing plan for a particular structure if required. 
· All viable material + framing plan alternatives must be considered and designed to compare the individual material + fabrication / erection costs to identify the most efficient and economical design for the structure. 
· For each material + framing plan alternative considered, designing the structure consists of designing the individual structural components, i.e., the members and the connections, of the framing plan. 
· This course CE470 focuses on the design of individual structural components. The material of construction will limited be steel, and the structural framing plans will be limited to braced frames and moment resisting frames. 

1.3 STRUCTURAL FRAMEWORK
· Figure 1 shows the structural plan and layout of a four-story office building to be located in West Lafayette. Figure 2 and 3 show the structural elevations of frames A-A and B-B, respectively, which are identified in Figure 1. 
[image: ]
[image: ]
[image: ]
· As shown in Figure 1, the building has two 25-ft. bays in the north-south direction and three 35 ft. bays in the east-west direction. 
· There are four structural frames in the north-south direction. These frames have structural elevations similar to frame A-A shown in Figure 2. 
· There are three structural frames in the east-west directions. These frames have structural elevations similar to frame B-B shown in Figure 3. 
· The building has a roof truss, which is shown in Figures 2 and 3. 
· Frame A-A is a braced frame, where all members are connected using pin/hinge connections. Diagonal bracing members are needed for stability. 
· Frame B-B is a moment frame, where all members are connected using fix/moment connections. There is no need for diagonal bracing members. 
· The north-south and east-west frames resist the vertical gravity loads together.
· The three moment frames in the east-west direction resist the horizontal lateral loads in the east-west direction. 
· The four braced frames in the north-south direction resist the horizontal lateral loads in the north-south direction.  

1.4 STRUCTURAL MEMBERS
Structural members are categorized based up on the internal forces in them. For example:
· Tension member –subjected to tensile axial force only
· Column or compression member –subjected to compressive axial force only
· Tension/Compression member –subjected to tensile/compressive axial forces
· Beam member –subjected to flexural loads, i.e., shear force and bending moment only. The axial force in a beam member is negligible. 
· Beam-column member – member subjected to combined axial force and flexural loads (shear force, and bending moments)

In basic structural analysis (CE371) students have come across two types of structures, namely, trusses and frames. For example, Figure 2 shows a roof truss supported by a braced frame. 

· All the members of a truss are connected using pin/hinge connections. All external forces are applied at the pins/hinges. As a result, all truss members are subjected to axial forces (tension or compression) only. 
· In braced and moment frames, the horizontal members (beams) are subjected to flexural loads only. 
· In braced frames, the vertical members (columns) are subjected to compressive axial forces only. 
·  In braced frames, the diagonal members (braces) are subjected to tension/compression axial forces only. 
· In moment frames, the vertical members (beam-columns) are subjected to combined axial and flexural loads. 

For practice, let us categorize the member shown in Figures 2 and 3. 
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1.5 STRUCTURAL CONNECTIONS
Members of a structural frame are connected together using connections. Prominent connection types include: (1) truss / bracing member connections; (2) simple shear connections; (3) fully-restrained moment connections; and (4) partially-restrained flexible moment connections. 
· Truss / bracing member connections are used to connect two or more truss members together. Only the axial forces in the members have to be transferred through the connection for continuity.
· Simple shear connections are the pin connections used to connect beam to column members. Only the shear forces are transferred through the connection for continuity. The bending moments are not transferred through the connection. 
· Moment connections are fix connections used to connect beam to column members. Both the shear forces and bending moments are transferred through the connections with very small deformations (full restraint). 
· Partially restrained connections are flexible connections used to connect beam to column members. The shear forces are transferred fully through the connection. However, the bending moment is only transferred partially. 
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Figure 5. Bracing connection and Simple Shear Connection at G in Frame A-A.
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Figure 6. All-bolted double angle shear connection.
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Figure 7. Directly welded flange fully restrained moment connection.




· Figure 4 shows an example truss connection. Figure 5 shows an example bracing connection. Figure 6 shows an example shear connection. Figure 7 shows an example moment connection. 
· Connections are developed using bolts or welds.
· Bolts are used to connect two or more plate elements that are in the same plane. Bolt-holes are drilled in the plate elements. The threaded bolt shank passes through the holes, and the connection is secured using nuts. 
· Bolts are usually made of higher strength steel.
· Welds can be used to connect plate elements that are in the same or different planes. A high voltage electric arc is developed between the two plate elements. The electric arc causes localized melting of the base metal (plate element) and the weld electrode. After cooling, all the molten metal (base and weld) solidifies into one continuum. Thus, developing a welded connection.
· In Figure 4, all the truss members are connected together by welding to a common gusset plate. The axial forces in the members are transferred through the gusset plates. This same connection can also be developed using bolts. How?
· In Figure 5, the bracing members are connected to gusset plates, which are also connected to the beam and column. The bracing member can be connected to the gusset plate using bolts or welds. However, the gusset plate has to be welded to the beam / column.
· In Figure 6, two angles are bolted to the web of the beam. The perpendicular legs of the angles are bolted to the flange of the column. Thus, an all-bolted double-angle shear connection is achieved. This all-bolted connection will be easier to assemble in the field as compared to welding. How is this a shear connection?
· In Figure 7, the beam flanges are beveled and welded directly to the flange of column using full penetration groove welds. This welding will have to be done in the field during erection and it will require the use of back-up bars. Weld-access holes and skilled welders are required to achieve a weld of acceptable quality.
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· In Figure 7, the beam web is bolted to a shear tab (plate), which is fillet welded to the column in the shop. This shear tab connection transfers the shear from the beam to the column.  How is Figure 7 a moment connection? 
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1.6 Structural Loads
The building structure must be designed to carry or resist the loads that are applied to it over its design-life. The building structure will be subjected to loads that have been categorized as follows:
· Dead Loads (D): are permanent loads acting on the structure. These include the self-weight of structural and non-structural components. They are usually gravity loads.
· Live Loads (L): are non-permanent loads acting on the structure due to its use and occupancy. The magnitude and location of live loads changes frequently over the design life. Hence, they cannot be estimated with the same accuracy as dead loads. 
· Wind Loads (W): are in the form of pressure or suction on the exterior surfaces of the building. They cause horizontal lateral loads (forces) on the structure, which can be critical for tall buildings. Wind loads also cause uplift of light roof systems.
· Snow Loads (S): are vertical gravity loads due to snow, which are subjected to variability due to seasons and drift.
· Roof Live Load (Lr): are live loads on the roof caused during the design life by planters, people, or by workers, equipment, and materials during maintenance. 
· Values of structural loads are given in the publication ASCE/SEI 7-10: Minimum Design Loads for Buildings and Other Structures. The first phase of structural design consists of estimating the loads acting on the structure. This is done using the load values and combinations presented in ASCE/SEI 7-10 as explained in the following sub-sections.


1.6.1 Step I. Categorization of Buildings
· Categories I, II, III, and IV. See Table 1.5-1 below and in ASCE/SEI 7-10.  [image: ]
1.6.2 Dead Loads (D)
Dead loads consist of the weight of all materials of construction incorporated into the building including but not limited to walls, floors, roofs, ceilings, stairways, built-in partitions, finishes, cladding and other similarly incorporated architectural and structural items, and fixed service equipment such as plumbing stacks and risers, electrical feeders, and heating, ventilating, and air conditioning systems.
In some cases, the structural dead load can be estimated satisfactorily from simple formulas based in the weights and sizes of similar structures. For example, the average weight of steel framed buildings is 60-75 lb/ft2, and the average weight for reinforced concrete buildings is 110 - 130 lb/ft2. 
From an engineering standpoint, once the materials and sizes of the various components of the structure are determined, their weights can be found from tables that list their densities. See Tables 1.2 and 1.3, which are taken from Hibbeler, R.C. (1999), Structural Analysis, 4th Edition. 
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1.6.3 Live Loads
· Building floors are usually subjected to uniform live loads or concentrated live loads. They have to be designed to safely support the minimum uniformly distributed load or the minimum concentrated live load values given in the ASCE/SEI 7-10 (see Table 4.1 below), whichever produces the maximum load effects in the structural members. 
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· The minimum uniformly distributed live loads (Lo) given in Table 4.1 above can be reduced for buildings with very large floor areas, because it is unlikely that the prescribed live load will occur simultaneously throughout the entire structure. 
· Equation (1.1) can be used to calculate the reduce uniformly distributed live load (L) for members with KLLAT≥400 ft2:

				(1.1)
where, AT is the tributary area in ft2 and KLL is the live load element factor as follows:
KLL is equal to 4.0 for interior columns and exterior columns without cantilever slabs. KLL is equal to 3.0 for edge columns with cantilever slabs.
KLL is equal to 2.0 for corner columns with cantilever slabs, edge beams without cantilever slabs, and interior beams.
KLL is equal to 1.0 for all other members not identified above.
EXCEPTION: Equation 1.1(a) can be used instead of Equation 1.1 for members of one and two-family structures supporting more than one floor load.

			(1.1(a))
Lo1, Lo2 … unreduced floor live load applicable to each of the supported story level irrespective of the tributary area.
L ≥ the largest unreduced floor live load on a given story level acting alone
· Some limitations to the live load reduction are as follows:
L cannot be less than 0.5Lo for members supporting one floor and L cannot be less that 0.4Lo for members supporting two or more floors.
Live loads that exceed 100 lb/ft2 shall not be reduced except the live loads for members supporting two or more floors may be reduced by 20%.
Live loads shall not be reduced for passenger vehicle garages except the live loads for members supporting two or more floors may be reduced by 20%.
Live loads shall not be reduced in assembly uses.
COMMENTARY on live loads from ASCE 7
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Example 1.1 Determine the magnitude and distribution of live loading on the north-south frame

bi - ei - hi

NOTES:

1)  The live loading on the beams bi - ei and ei – hi can be calculated using the reduced floor live load and the tributary area for the beams supporting the floors.

2)  The live loads acting on beams di – ei and ei - fi can be used to determine the concentrated live load reactions on columns di, ei, and fi
-	Where, the live loads acting on the beams di – ei and ei - fi are calculated using the reduced floor live load and the corresponding tributary area for the beams

3)  The concentrated live load acting on the columns can also be estimated directly using the reduced live load and the tributary area for the columns.

-	But, this method would be inconsistent because the live load carried by the beams bi-ei

and ei-hi would be included twice.

-	Additionally, the live load reduction factor calculated directly for the columns will be different from the live load reduction factors calculated for the beams. Consider the Tables developed in this example.

•	Step I: Determine relevant tributary and influence areas. Estimate live load reduction factors.
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Table 1.1 Member tributary areas and minimum design live loading.

	Beam

Member
	Tributary area
	KLL
	L/Lo=0.25 + 15.0/(KLLAT)0.5
	L/Lo min.

	bi-ei

ei-hi
	AT = ½ x 25.0 x 12.5 x 2
= 312.5 ft2
	2.0
	0.85
	0.5

	
	
	
	
	

	di - ei

ei - fi
	AT = ½ x 12.5 x 25.0 x 2 +
25.0 x 25.0 = 937.5 ft2
	2.0
	0.60
	0.5

	
	
	
	
	

	gi - hi

hi - ii ai - bi bi - ci
	

AT = ½ x (50+25) x 12.5
= 468.75 ft2
	

2.0
	

0.74
	

0.5

	
	
	
	
	

	ai - di

di - gi ci - fi fi - ii
	

AT = ½ x 25.0 x 12.5
= 156.25 ft2
	



2.0
	



1.0
	



0.5

	
	
	
	
	




Step II. Estimate the distributed loads acting on the beams bi - ei and ei - hi



b6 	e6

b5 	e5

h6 	(0.85x50 x25)/1000=1.06k/ft.

h5



b4 	e4

b3 	e3

b2 	e2

bi 	ei
h4


h3


h2


b1 	e1 	h1



Step III: Estimate the concentrated live loads acting on the columns of frame bi-ei-hi, which are produced by the live load distribution on the beams of the orthogonal frames di-ei-fi , ai-bi-ci , and
gi-hi-ii





d6 	e6



28.125 k

(0.60x50x25)/1000=0.75k/ft.

f6




d5 	e5

d4 	e4


d3 	e3

d2 	e2


28.125 k


28.125 k


28.125 k


Resultant
28.125 k

f5

12.5’
f4 	14.0625 k

f3

f2



25’ 	12.5’



0.60x50x25=0.75k/ft.





14.0625 k


d1 	e1 	f1



12.5’
14.0625 k



25’ 	12.5’
14.0625 k





a6 	b6  17.34 k

a5

0.74x50 x12.5=0.46k/ft
c6

c5

b5  17.34 k
a4b

4  17.34 k

a3



c4 	12.5’
8.67 k

c3



25’ 	12.5’




8. 67 k

b3

a2 	b2

a1

b1

17.34 k


Resultant
17.34 k



c2

c1

12.5’
8.67 k

0.74x50 x12.5=0.46k/ft






25’ 	12.5’
8.67 k

 

Thus, the concentrated live loads acting on columns bi and hi are 17.34 kips

The concentrated live loads acting on columns ei are 28.125 k



Step IV: Check the estimated column live loadings with values that would be obtained directly

for the columns


hi
gi
AT = 12.5 x 50 = 625 ft2



A  = 25 x 50 = 1250 ft2T

di

ei



ii



25 ft.



fi








ai


50 ft.



AT = 12.5 x 50 = 625 ft2

bi

50 ft.

25 ft.



ci



	Column

Member
	Tributary area
	KLL
	L/Lo=0.25 + 15.0/(KLLAT)0.5
	L/Lo min.

	bi

hi
	AT = 12.5 x 50 = 625 ft2
	4.0
	0.55
	0.4

0.5 for b6, h6

	
	
	
	
	

	ei
	AT = 25 x 50 = 1250 ft2
	4.0
	0.46
	0.4

0.5 for e6

	
	
	
	
	




Live load acting on column bi and hi are = 0.55 x 50 psf x 625 = 17.18 kips

Live load acting on column ei = 0.46 x 50 psf x 1250 = 28.75 kips

-	Live load acting on column e6 = 0.5 x 50 psf x 1250 = 31.25 kips

•	Note that the live loads calculated in Steps I, II, and III are consistent and to be used for design.

•	The concentrated live load calculated in Step IV are just to check that the loads calculated in Steps I, II, and III are more than the loads calculated in Step IV.

[bookmark: _GoBack]Example 1.2 Determine the magnitude and distribution of live loading on the north-south frame . bi - ei - hi. Note the different dimensions etc. This is not the same problem as the preview one.

Step I: Determine relevant tributary and influence areas. Estimate live load reduction factors.
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Table 1.1 Member tributary areas and minimum design live loading.

	Beam

Member
	Tributary area
	KLL
	L/Lo=0.25 + 15.0/(KLLAT)0.5
	L/Lo min.

	di-ei

ei-fi

and other internal beams
	AT = 40 x 6.0
= 240.0 ft2
	2.0
	0.94
	0.5

	
	
	
	
	

	gi –hi and hi - ii

ai-bi and bi-ci
	

AT = 40 x 3.0
= 120.0 ft2
	2.0
	1.0
	0.5

	
	
	
	
	





Step II. Estimate the distributed loads acting on the beams: (i) di-ei and ei-fi, (ii) ai-bi and bi-ci, and (iii) gi-hi and hi-ii
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Step III: Estimate the concentrated live loads acting on the beams and columns of frame bi-ei-hi 
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Step IV – Checking the Column Reduced Live Load 


	Column

Member
	Tributary area
	KLL
	L/Lo=0.25 + 15.0/(KLLAT)0.5
	L/Lo min.

	bi

hi
	AT = 15 x 40 = 600 ft2
	4.0
	0.56
	0.4

0.5 for b6, h6

	
	
	
	
	

	ei
	AT = 30 x 40 = 1200 ft2
	4.0
	0.47
	0.4

0.5 for e6

	
	
	
	
	




Live load acting on column bi and hi are = 0.56 x 50 psf x 600 = 16.8 kips

Live load acting on column ei = 0.47 x 50 psf x 1200 = 28.20 kips

-	Live load acting on column e6 = 0.5 x 50 psf x 1200 = 30.0 kips

Note that the live loads calculated in Steps I, II, and III are consistent and to be used for design.

•The concentrated live load calculated in Step IV are just to check that the loads calculated in Steps I, II, and III are more than the loads calculated in Step IV.



1.6.4 Roof Live Loads
Ordinary flat, pitched, and curved roofs shall be designed for the live loads specified in Equation 1.2 (from ASCE/SEI 7-10). 
Lr = 20 R1 R2 		where, 12 ≤ Lr ≤ 20 			(1.2)
where, 
Lr is the roof live load per square foot of horizontal projection in psf.
= 1 			for AT ≤ 200 ft2
 R1 	= 1.2 - 0.001 AT 	for 200 < AT < 600 ft2
	= 0.6 			for 600ft2 ≤ AT
____________________________________________________________________
	= 1 			for F ≤ 4
R2	= 1.2 - 0.05 F		for 4 < F < 12		
	= 0.6 			for 12 ≤ F
where, F = no. of inches of rise per foot for pitched roof. 1.6.5 Wind Loads


· Design wind loads for buildings can be based on: (a) simplified procedure; (b) analytical procedure; and (c) wind tunnel or small-scale procedure.
· Figure 26.1-1 (ASCE/SEI 7-10) outlines the process for determining wind loads. 
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· Refer to ASCE/SEI 7-10 for the simplified procedure. This simplified procedure is applicable only to buildings with mean roof height less than 30 ft. 
· The wind tunnel procedure consists of developing a small-scale model of the building and testing it in a wind tunnel to determine the expected wind pressures etc. It is expensive and may be utilized for difficult or special situations.
· The analytical procedure is used in most design offices. It is fairly systematic but somewhat complicated to account for the various situations that can occur.
· Wind velocity will cause pressure on any surface in its path. The wind velocity and hence the velocity pressure depend on the height from the ground level. Equation 1.3 is recommended by ASCE/SEI 7-10 (Equation 27.3-1) for calculating the velocity pressure (qz) in lb/ft2 
qz = 0.00256 Kz Kzt Kd V2      (lb/ft2)			(1.3)
where, V is the basic wind speed 		(see Figure 26.5-1 in ASCE/SEI 7-10 )
	Kd is a wind directionality factor 	(=0.85 for CE 470)
	Kzt is a topographic factor  		(= 1.0 for CE 470)
	Kz varies with height z above the ground level and Exposure category (see Table 27.3-1 in ASCE/SEI 7-10 )
· Basic Wind Speed (V) : 
· For Risk Category II buildings and structures – use Fig. 26.5-1A
· For Risk Category III and IV buildings and structures – use Fig. 26.5-1B
· For Risk Category I buildings and structures – use Fig. 26.5-1C
· A significant portion of the U.S. including West Lafayette has V = 115 mph for Risk Category II (Fig. 26.5-1A). At these locations, for Risk Category II
qz = 28.78 Kz	(lb/ft2)				(1.4)
· 
The velocity pressure qz is used to calculate the design wind pressure (p) for the building structure as follows:
p = q GCp – qi (GCpi)	 	(lb/ft2)			(1.5) 
where, G = gust effect factor (=0.85 for CE 470)
Cp = external pressure coefficient from Figures 27.4-1, 27.4-2 and 27.4-3in ASCE/SEI 7-10 
	(GCpi )= internal pressure coefficient from Table 26.11-1 in ASCE/SEI 7-10 
q depends on the orientation of the building wall or roof with respect to direction of the wind as follows:
q = qz 	for the windward wall – varies with height z
	q = qh 	for leeward wall. 
qh 	is qz evaluated at z = h (mean height of building). qh is constant.
qi = qh  for windward, leeward, side walls and roofs (fully enclosed building)

· Note that a positive sign indicates pressure acting towards a surface. Negative sign indicate pressure away from the surface
· Equation 1.5 indicates that the design wind pressure p consists of two components: (1) the external pressure on the building (q GCp); and (2) the internal pressure in the building (qiGCpi)








ASCE/SEI 7-10 Figure 26.8-1 (Pg. 252-253)
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Figure showing the Basic Wind Speed map of US (Category II Buildings). (ASCE/SEI 7-10 Pages 290-291)
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External Pressure Coefficients Figures 27.4-1, 2 &3 (ASCE/SEI 7-10 Pages.263-266) 
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Wind Directionality Factor (ASCE/SEI 7-10 Page 250)
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Velocity Pressure Exposure Coefficient (ASCE/SEI 7-10, Page 261)
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Internal Pressure Coefficient for buildings (ASCE/SEI 7-10. Page 258)
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Example 1.2
Consider the building structure with the structural floor plan and elevation shown below. Estimate the wind loads acting on the structure when the wind blows in the east-west direction. The structure is located in West Lafayette.
[image: ]
Figure 8. Structural floor plan
[image: ]
Figure 9. Structural elevation in east-west direction
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                    Figure 10. Structural elevation in north-south direction
· Velocity pressure (qz)
· Kd = directionality factor = 0.85
· Kzt = topographic factor = 1.0
· Kh values for Exposure B, Case 2
	Kh
	z(ft)

	 0.57
	0 - 15

	0.62
	20

	0.66
	25

	0.70
	30

	0.76
	40

	0.81
	50

	0.85
	60

	0.89
	70



· qz = 0.00256 Kz Kzt Kd V2
· In West Lafayette, V = 115 mph for Risk Category II (Fig. 26.5-1A)
· qz = 28.78 Kz psf
· Wind pressure (p)
· Gust factor = G = 0.85
· For wind in east west direction; L/B = Length / width = 2.0
· External pressure coefficient = Cp = +0.8 for windward walls	
  Cp = -0.3 for leeward walls
  Cp = -0.7 for side walls
· External pressure = q G Cp
· External pressure on windward wall = qz GCp = 28.78 Kz x 0.85 x 0.8 
  = 19.57 Kz psf toward surface
· External pressure on leeward wall = qh GCp 	= 28.78 K65 x 0.85 x (-0.3)
= 6.38 psf away from surface
· External pressure on side wall = qh GCp	=28.78 K65 x 0.85 x (-0.7)
= 14.90 psf away from surface
· The external pressures on the structure are shown in Figures 11 and 12 below.
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Figure 11. External pressures on structural plan 
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Figure 12. External pressure on structural elevation (east west)
· Internal pressure 
· qi (GCpi)
· qi = qh = 28.78 K65 = 28.78 x 0.87 = 25.04 psf
· Enclosed building; 	GCpi = +0.18  (acting toward surface)
GCpi = -0.18 (acting away from surface)
· qi (GCpi) = 4.51 psf acting toward  or away from surface
· See Figure 13 (a) and (b) below
(a)						(b)
[image: ][image: ]
Figure 13. Internal pressure seen in structural plan
· Take the external pressure from Figure 11 and 12 and add to internal pressure from Figures 13 (a) and (b) to obtain the final pressure diagrams. Adding the internal pressure will not change the lateral forces in the structure. 

  			(a)						(b)
[image: ][image: ]
Figure 14. Resultant wind pressure diagrams including external and internal pressures
· Note: According to ASCE/SEI 7-10, the minimum wind design loading is equal to 16 lb/ft2 multiplied by the area of the building projected on a vertical plane normal to assumed wind direction. 
· Compare the determined design wind loading with the minimum value and continue with the greater as the design wind loading..
1.7 Load and Resistance Factor Design 
	The load and resistance factor design approach is recommended by AISC for designing steel structures. It can be understood as follows:
Step I. Determine the ultimate loads acting on the structure
· The values of D, L, W, etc. given by ASCE/SEI 7-10 are nominal loads (not maximum or ultimate)
· During its design life, a structure can be subjected to some maximum or ultimate loads caused by combinations of D, L, or W loading.
· The ultimate load on the structure can be calculated using factored load combinations, which are given by ASCE and AISC (see pages 2-10 and 2-11 of AISC manual). The most relevant of these load combinations are given below:
1.4 D					(1.6 – 1)
1.2 D + 1.6 L + 0.5 (Lr or S)			(1.6 – 2)
1.2 D + 1.6 (Lr or S) + (0.5 L or 0.5 W)			(1.6 – 3)
1.2 D + 1.0W + 0.5 L + 0.5 (Lr or S)			(1.6 – 4)
0.9 D + 1.0 W				(1.6 – 5)
Step II. Conduct linear elastic structural analysis
· Determine the design forces (Pu, Vu, and Mu) for each structural member

Step III. Design the members
· The failure (design) strength of the designed member must be greater than the corresponding design forces calculated in Step II. See Equation (1.7) below: 

		 			 Rn > 				(1.7)
· Where, Rn is the calculated failure strength of the member
·  is the resistance factor used to account for the reliability of the material behavior and equations for Rn
· Qi is the nominal load
· i is the load factor used to account for the variability in loading and to estimate the ultimate loading condition.
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Table 1-2 Minimum Densities for Design Loads from Table 1-3 Minimum Design Dead Loads*
Materials*

i 5 Walls psf N/m?
To/ft N/m 4-in. (102 mm) clay brick 39 187
Aluminum 170 2.7 8-in. (203 mm) clay brick 79 3.78
12-in. (305 mm) clay brick 115 5.51
in ci 17.0
Concrete, plain cinder 108 Frame Partitions and Walls
Concrete, plain stone 144 226 Exterior stud walls with brick veneer 48 230
Concrete, reinforced cinder 111 174 Windows, glass, frame and sash 8 038
Wood studs 2 X 4, (51 X 102)
Concrete, reinforced stone 150 236 unplastered 4 019
Wood studs 2 X 4, (51 X 102)
Clay, dry 6 99 plastered one side 12 057
Clay, damp 110 173 Wood studs 2 X 4, (51 X 102)
plastered two sides 20 096
Sand and gravel, dry, loose 100 157 )
Floor Fill
Sand and gravel, wet 120 B8 Cinder concrete, per inch (mm) 9 0017
Masonry, lightweight solid concrete 105 165 Lightweight concrete, plain,
) - per inch (mm) 8 0015
Masonry, normal weight 135 212 Stone concrete, per inch (mm) 12 0.023
Plywood 36 5.7 Ceilings
Steel, cold-drawn 492 713 Acoustical fiberboard 1 0.05
. Plaster on tile or concrete 5 0.24
‘Wood, Douglas Fir 34 53 Suspended metal lath and gypsum
. laster 10 048
Wood, Southern Pine 37 58 ks
! Asphalt shingles 2 010
Wood, spruce 29 45 Fiberboard, J-in. (13 mm) 0.75 0.04

*Reproduced with permission from American Society of Civil Engineers Minimum Design Loads for Buildings and Other Siructures, ANSI/ASCE 7-95. Copies of this
standard may be purchased from ASCE at 345 East 47th Street, New York, N.Y. 10017-2398.
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It is well known that the floor loads measured in a live-load
survey usually are well below present design values [Refs. C4-
2, C4-3, C4-4, C4-5). However, buildings must be designed to
resist the maximum loads they are likely to be subjected to
during some reference period T, frequently taken as S0 years.
Table C4-2 bricfly summarizes how load survey data are com-
bined with a theoreti s of the load process for some
common occupancy types and illustrates how a design load might
be selected for an occupancy not specified in Table 4-1 [Ref. C4-
6]. The floor load normally present for the intended functions of
a given occupancy is referred to as the sustained load. This load
is modeled as constant until a change in tenant or occupancy type.
occurs. A live-load survey provides the statistics of the sustained
load. Table C4-2 gives the mean, m, and
oy, for particular reference a . In addition to the sus
load, a building i likely to be subjected to a number of relatively
short-duration, high-intensity, extraordinary, or transient loading
events (due 1o crowding in special or emergency circumstances,
concentrations during remodeling, and the like). Limited survey
information and theoretical considerations lead to the means, m,,
and standard deviations, o;, of single transient loads shown in
Table C4-2.

Combination of the sustained load and transient load proce:
with due regard for the probabilities of occurrence, leads to statis
tics of the maximum total load during a specified reference period
7. The statistics of the maximum total load depend on the average
duration of an individual tenancy, 7, the mean rate of occurrence
of the transient load, v,, and the reference period, 7. Mean va
ues are given in Table C4-2. The mean of the maximum load is
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TABLE C4-2 TYPICAL LIVE LOAD STATISTICS

Survey Load Transient Load “Temporal Constants Mean
maximum
Occupancy me i e a u* e T Toad*
or use I/ (KN/m?) Ibvf? (KN/m?) Ib/AE (KN/m?) Ib/f? (KN/m?) (years) (per year) (years) bV (KN/m?)
Office buildings
offices 109 052) 59(028) 80038) 82(039) 8 1 50 55(2.6%)
Residential
renter occupied 60029) 26(0.12) 60029) 2) 2 1 50 36(1.72)
owner occupied 60029) 2610.12) 60029) 2) 10 i 50
Hotels
guest rooms 45022) 12006) 60(029) 58(028) s 20 50 4622)
Schools
classrooms 120057 27013 69033) 34(0.16) 1 1 100 34(1.63)

For 200 f* (18.58 m?) area. except 1000 fi? (92.9 m?) for schools.
* Duration of average sustained load occupancy.

“Mean rate of occurrence of transient load.

“Reference period.
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Figure 1. Structural floor plan and layout
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Figure 2. Structural elevation of frame A-A

A

B

C

D

E

F

G

H

I

J

K

L

M

N

O

P

Q

R

S

T

10 ft.

12 ft.

12 ft.

12 ft.

15 ft.

10 ft.

12 ft.

12 ft.

12 ft.

15 ft.

25 ft. 25 ft.

Figure 2. Structural elevation of frame A-A

A

B

C

D

E

F

G

H

I

J

K

L

M

N

O

P

Q

R

S

T


image69.png




image70.png




image71.png




image72.png




image73.png




image74.png




image75.png




image76.png




image77.png




image78.png




